Doc. ECC(14)008 Annex 01 Bis

Outline of CEPT Response

The outline of the response to the Commission in respect of the development of a CEPT response to the EC Mandate “To undertake studies on the harmonised technical conditions for the 1900-1920 MHz and 2010-2025 MHz frequency bands (“Unpaired terrestrial 2 GHz bands”) in the EU”

**DD March 2014**

**FOREWORD**

The present outline of the response to the Commission describes the shortlist of potential harmonised uses of the 1900-1920 MHz and 2010-2025 MHz frequency bands in accordance with the EC Mandate to CEPT “To undertake studies on the harmonised technical conditions for the 1900-1920 MHz and 2010-2025 MHz frequency bands (“Unpaired terrestrial 2 GHz bands”) in the EU”.

The full range of source information has not been available to the extent that an ECC consultation in the formal sense could have been started at the ECC meeting in 5-8 November 2013. Therefore, the ECC decided instead to make a ‘Call for Inputs’ in order to gather relevant information from stakeholders in a timescale aligned with the requirements of the “Unpaired terrestrial 2 GHz bands” mandate.

A summary of the responses to the Call for Inputs, as well as the responses received during the consultation period, are presented in Annex 2.

The CEPT’s final response to the EC Mandate on the “Unpaired terrestrial 2 GHz bands” is currently under development and will include the present outline of the response to the Commission describing the shortlist of potential harmonised uses of the 1900-1920  MHz and 2010-2025 MHz frequency bands (tasks 1 and 2) as well as more information in response to task 3 as required under the Mandate.

A Public Consultation on the CEPT’s response to the EC Mandate (draft CEPT Report) will take place in June 2014 in response to the Mandate.

# Executive summary

The outline of the response to the Commission has been developed within European Conference of Postal and Telecommunications Administrations (CEPT) in the framework of the EC mandate to assess and identify alternative uses of the unpaired terrestrial 2 GHz frequency bands (1900-1920 MHz and 2010-2025 MHz) other than for the provision of mobile electronic communications services through terrestrial cellular networks (as introduced by the UMTS Decision) as well as develop relevant least restrictive technical conditions for spectrum use.

The European Commission considered that there is no viable harmonisation option within the mobile broadband context for the unpaired terrestrial 2 GHz spectrum that would have a limited or no impact on current licences. An alternative harmonisation option outside the current framework of licence conditions would have to be pursued, which would likely to imply change or revocation of existing authorisations.

Therefore, CEPT was mandated to undertake the following tasks:

1. Assess and identify uses other than mobile electronic communications services delivered through terrestrial cellular networks and define the common minimal (least restrictive) technical conditions. These conditions should be sufficient to avoid interference with services or radio applications in adjacent bands, ensure coexistence with other services or radio applications in the same band, and facilitate cross-border coordination, also at the EU outer borders;
2. In performing task (1), consider the following non-ECS uses in line with the priorities of the RSPP: broadband PPDR, PMSE, short-range devices and DECT. This is without prejudice to the consideration of alternative uses for electronic communications services in line with EU spectrum policy objectives, such as Broadband Direct-Air-To-Ground Communications;
3. In performing task (1) as specified by task (2) and given the limited temporal or geographical scope of one or more of the radio application under consideration, assess and justify the possibility of spectrum sharing amongst the radio applications under consideration and, if necessary, develop common technical sharing conditions which may include inter alia spectrum access rules, channelling arrangements or power emission limits that are sufficiently precise for the development of EU-wide equipment.

After performing the analysis described in the outline of the response to the Commission, the following harmonisation possibilities were obtained:

As presented in section 2.2 (Current authorisations and uses of the unpaired 2 GHz bands), there are licences in force in Europe in both unpaired 2 GHz bands. Some of the licences were awarded after spectrum auction processes and, as a result, considerable auction prices were achieved. In some countries, a licence repeal process might be possible in case of continued non-implementation, whereas in other countries this will not be possible due to specific conditions and obligations which are part of the licence (e.g., coverage obligations are interpreted in some cases as fulfilled when providing services via other spectrum where the same licensee has also a licence and for which the network is implemented). Other options for making the spectrum available for new usage need to be considered (e.g. liberalisation, transfer).

A Broadband DA2GC system constitutes an application for various types of telecommunications services, such as internet access and mobile multimedia services (described in section 3.1). It aims to provide access to broadband communication services during continental flights on a Europe-wide basis. Currently, there is no spectrum designated for Broadband DA2GC in Europe. To allow European citizens and airlines to profit from the social and economic benefits of the implementation of such a radio application (intended to provide broadband connectivity between the aircraft and a terrestrial based network), a harmonised spectrum designation within CEPT would be necessary. In order for the system to be commercially viable it would need to have the potential to provide a pan-European solution.

With respect to PMSE (section 3.2), it is considered that there is a need for these services to be coordinated to avoid harmful interference and therefore an individual authorisation regime may be appropriate for implementation by national administrations.

Concerning SRD applications (section 3.3), no allocations are required for SRD to operate in a specific frequency band (SRD typically operate on a non-interference and non-protection basis). A simple request from industry would be taken into account at any time but preferably, when a primary usage is identified.

Regarding the proposal for DECT as set out in section 3.4, if realised under application-neutral and technology-neutral principles (see CEPT Report 014 [1] and CEPT Report 044 [2]) using general authorisation (exemption from individual licence), this can also be regarded as a new spectrum opportunity for SRD usage, provided that suitable spectrum access rules are followed.

A harmonised solution for ad-hoc PPDR network uses above 1 GHz is under consideration, which includes, for some countries, PPDR broadband air-to-ground applications (section 3.5). Cross-border coordination is needed for PPDR broadband air-to-ground applications. Broadband PPDR temporary additional capacity (also known as “hot-spot” or “local area” networks) are supposed to provide additional local coverage at the scene of the incident in order to provide the necessary communication facilities to PPDR users in addition to those provided through the Wide Area network (WAN) or where the WAN radiocommunications are limited or not available. This additional capacity may be provided by Ad-hoc networks or other means (such as additional temporary base stations of the WAN) and are supposed to have high capacity and support PPDR users with low mobility. Ad-hoc networks may operate in the same (i.e. in a form of an ad-hoc micro-cell deployed at the event’s scene) as well as in a different frequency band.

PMSE use described in section 3.2 (Programme Making and Special Events) and ad-hoc PPDR use identified in section 3.5 (Public Protection and Disaster Relief) are further explored, since the same technologies / equipment may be used and the same technical framework might apply.

In this outline of the response to the Commission it is therefore suggested placing the shortlist of potential harmonised uses of the 1900-1920 MHz and 2010-2025 MHz frequency bands proposed for further study in the EC Mandate (as detailed in Annex 1) into 3 defined categories:

* Direct air to ground communications
* Video links and cordless cameras (PMSE / ad-hoc PPDR)
* Applications under general authorisation (DECT / SRD)

The objective of proceeding with these 3 categories is to take advantage of the synergies between the above identified uses by sharing the same technical framework to foster a more efficient use of spectrum and future innovation.

A high level of support was expressed in the responses to the Call for Inputs for placing the shortlist of potential harmonised uses of the 1900-1920 MHz and 2010-2025 MHz frequency bands (as proposed for further study in the EC Mandate) into the above 3 categories, although it became visible from the contributions that it was desirable to further investigate and clarify the technical characteristics and usage conditions for specific candidate applications during the development of the final CEPT Report.

**TABLE OF CONTENTS**

[0 Executive summary 3](#_Toc378073653)

[1 introduction 8](#_Toc378073654)

[2 BACKGROUND INFORMATION 9](#_Toc378073655)

[2.1 Current regulatory framework in CEPT 9](#_Toc378073656)

[2.2 Current authorisations and uses of the unpaired 2 GHz bands 10](#_Toc378073657)

[2.3 Current use and regulatory framework outside CEPT 11](#_Toc378073658)

[2.4 Previous studies on the unpaired 2 GHz bands 15](#_Toc378073659)

[2.5 Identification of alternative uses for both unpaired 2 GHz bands 15](#_Toc378073660)

[3 ALTERNATIVE USES INCLUDING SPECTRUM REQUIREMENTS 17](#_Toc378073661)

[3.1 Broadband Direct Air to Ground Communications 17](#_Toc378073662)

[3.2 Programme Making and Special Events 23](#_Toc378073663)

[3.3 Short Range Devices 25](#_Toc378073664)

[3.4 Digital Enhanced Cordless Telecommunications 26](#_Toc378073665)

[3.5 Public Protection and Disaster Relief 28](#_Toc378073666)

[3.6 Synergies between the proposed short list of selected use 28](#_Toc378073667)

[ANNEX 1: EC Mandate 31](#_Toc378073668)

[ANNEX 2: RESULTS OF THE CALL FOR INPUTS 36](#_Toc378073669)

[ANNEX 3: Current authorisations in the bands 1900-1920 MHz / 2010-2025 MHz 41](#_Toc378073670)

[ANNEX 4: Typical Technical Characteristics for ENG/OB Links (Extracted from ERC Recommendation 25-10) 51](#_Toc378073671)

[ANNEX 5: Typical Technical Characteristics for ENG/OB Links (Extracted from ERC Report 38 52](#_Toc378073672)

[ANNEX 6: List of references 53](#_Toc378073673)

**LIST OF ABBREVIATIONS**

|  |  |
| --- | --- |
| **Abbreviation** | **Explanation** |
| **AS** | Aircraft Station |
| **CAA**  **CEPT** | Civil Aviation Administration  European Conference of Postal and Telecommunications Administrations |
| **CDMA**  **DA2GC**  **DECT** | Code Division Multiple Access  Direct-Air-to-Ground Communications  Digital Enhanced Cordless Telecommunications |
| **EC** | European Commission |
| **ECA** | European Common Allocation |
| **ECC** | Electronic Communications Committee |
| **ECO** | European Communications Office |
| **ECS** | Electronic Communications Services |
| **EESS**  **EFIS**  **ERC**  **ESOMPs** | Earth Exploration-Satellite Service  ECO Frequency Information System  European Radio Committee (superseded by ECC)  Earth Stations On Mobile Platforms |
| **ETSI** | European Telecommunications Standards Institute |
| **EU**  **FCC** | European Union  Federal Communication Commission |
| **FDD** | Frequency Division Duplex |
| **FL** | Forward Link |
| **FS**  **FSS**  **FWA**  **GS**  **GSMOBA** | Fixed Service  Fixed Satellite Service  Fixed Wireless Access  Ground Station  GSM On-board Aircraft |
| **IMT** | International Mobile Telecommunications |
| **LTE**  **MSS**  **MVL**  **NTFA**  **OFDMA**  **OPEX** | Long Term Evolution  Mobile Satellite Service  Mobile Video Links  National Table of Frequency Allocations  Orthogonal Frequency Division Multiple Access  Operating Expenses |
| **PHS** | Personal Handyphone System |
| **PMSE** | Programme Making and Special Events |
| **PPDR** | Public Protection and Disaster Relief |
| **QAM** | Quadrature Amplitude Modulation |
| **RF** | Radio Frequency |
| **RL** | Reverse Link |
| **RSC** | Radio Spectrum Committee |
| **RSPG** | Radio Spectrum Policy Group |
| **RSPP** | Radio Spectrum Policy Programme |
| **R&TTE**  **SAB/SAP** | Radio Equipment and Telecommunications Terminal Equipment  Services Ancillary to Broadcasting / Services Ancillary to Programme making |
| **SOS**  **SRD**  **SRDoc**  **SRS**  **TDD**  **TRR** | Space Operation Service  Short Range Devices  ETSI System Reference Document  Space Research Service  Time Division Duplex  Tactical Radio Relay |
| **UHF**  **ULE**  **UMTS**  **WAN**  **WG FM**  **WLL** | Ultra High Frequencies  Ultra Low Energy  Universal Mobile Telecommunications System  Wireless Area Networks  Working Group Frequency Management  Wireless Local Loop |
| **WRC** | World Radio Conference |
|  |  |

# introduction

The use of the unpaired terrestrial 2 GHz frequency bands, 1900-1920 MHz and 2010-2025 MHz, was established within CEPT for IMT-2000/UMTS more than 10 years ago. These frequency bands, originally planned for TDD use, were later harmonised to allow greater flexibility in the use of the bands   
1900-1920 MHz and 2010-2025 MHz for either TDD or FDD uplink (to be paired with another band). This harmonisation, as part of a process of making available spectrum for future mobile telecommunications systems within CEPT, has been the basis of a number of authorisations that have been granted for the bands 1900-1920 MHz and 2010-2025 MHz.

CEPT analysed the usage of the unpaired terrestrial 2 GHz bands and came to the conclusion that those bands were mostly unused. In summary, the band 1900-1920 MHz, although licensed in many countries, remained largely unused, and the use of frequencies in the band 2010-2025 MHz had only been authorised in few countries.

The pairing of 1900/1905-1920 MHz with 2090/2095-2110 MHz, as well as an internal pairing of 1900-1920 MHz with 2010-2025 MHz (limiting the pairing to 2x15 MHz), or even external pairing, were investigated within CEPT for cellular mobile mass market applications but considered inappropriate. Increased complexity (additional bands) in User Equipment (UE) design compared to very limited benefits for the cellular mobile community led to lack of support from Industry.

Thus, further investigations were considered needed to develop a suitable ECC framework for those bands, focusing on alternative uses in the unpaired sub-bands (1900-1920 MHz and 2010-2025 MHz) other than for the provision of mobile electronic communications services through terrestrial cellular networks.

At the end of 2012, CEPT was mandated to assess and identify alternative uses of the unpaired terrestrial  
2 GHz frequency bands (1900-1920 MHz and 2010-2025 MHz) other than for the provision of mobile electronic communications services through terrestrial cellular networks (as introduced by the UMTS Decision) as well as to develop least restrictive technical conditions for their deployment while ensuring co-existence with the electronic communications services in the paired 2 GHz spectrum.

The outline of the response to the Commission is intended to describe the work undertaken so far. In particular, it gives an overview of CEPT investigations on alternative uses of bands 1900-1920 MHz and 2010-2025 MHz, other than for the provision of mobile electronic communications services through terrestrial cellular networks.

# BACKGROUND INFORMATION

## Current regulatory framework in CEPT

The bands 1885-2025 MHz and 2110-2170 MHz were identified for International Mobile Telecommunications – 2000 (IMT-2000) in the World Administrative Radiocommunications Conference held in 1992 (WARC-92) through footnote 5.388 of the Radio Regulations (RR). These bands include the satellite component of IMT-2000.

Within the IMT-2000 family, the Universal Mobile Telecommunications Systems (UMTS) terrestrial radio access (UTRA) has been developed with 2 modes of operation ([http://www.itu.int/osg/spu/ni/3G/technology/#Cellular](http://www.itu.int/osg/spu/ni/3G/technology/%23Cellular) Standards for the Third Generation); a Frequency Division Duplex (FDD) mode and a Time Division Duplex (TDD) mode. The FDD mode provides efficient operation in many UMTS environments, providing wide area coverage and full mobility applications. The TDD mode however may allow operators flexibility in network deployment and to support traffic asymmetry in an efficient way.

In 1997, CEPT identified in ERC/DEC/(97)07 [5] the core frequency bands for UMTS in Europe. This Decision designated 155 MHz of spectrum to terrestrial UMTS applications with an additional 60 MHz for UMTS satellite services. In Europe, the 15 MHz spectrum at 1885-1900 MHz identified by WARC-92 for IMT-2000 was not designated for UMTS in ERC/DEC/(97)07 [5] due to current usage of this band by Digital Enhanced Cordless Telecommunications (DECT). The Decision required that administrations make available at least 2x40 MHz from within these bands by 2002.

Decision 128/1999/EC [8] of the European Parliament and the Council, dated 14 December 1998, on the coordinated introduction of a third-generation mobile and wireless communications system (UMTS) in the Community, came into force at the begin of 1999 with the aim to facilitate the rapid and coordinated introduction of compatible UMTS networks and services in the Community on the basis of internal market principles and in accordance with commercial demand.

In November 1999, ERC adopted Decision ERC/DEC/(99)25 [3], on the harmonised utilisation of spectrum for terrestrial UMTS operating within the bands 1900-1980 MHz, 2010-2025 MHz and 2110-2170 MHz. This Decision requested that, subject to market demand, administrations make provisions to allow the operation of UMTS self provided applications in a self-coordinating mode in the frequency band 2010-2020 MHz. It also indicated that the designation of this band for UMTS self provided applications may be reviewed two years after the date of entry into force.

In response to Mandate 1 of the European Commission to CEPT, ERC/DEC/(00)01 [4] extended ERC/DEC/(97)07 [5] to require that administrations make available the entire 155 MHz of terrestrial spectrum for UMTS and other systems included in the IMT-2000 family by 1 January 2002, subject to geographical spread market demand and national licensing schemes.

More than five years after the entry into force of ERC/DEC/(99)25 [3], it has become clear that the anticipated market for UMTS self provided applications has not materialised. It was also noted that there was a desire amongst some administrations and operators to allow greater flexibility in the use of the bands 1900-1920 MHz and 2010-2025 MHz, with the choice between FDD uplink and TDD mode being made subject to market demand on a national basis. In December 2004 the European Union sent a liaison statement to CEPT highlighting the results of a questionnaire to Member States on use of the band 2010-2025 MHz, indicating “… that there does not seem to be any interest for self provided applications which are currently foreseen in the band 2010-2020 MHz…”.

In 2006 a new ECC Decision, ECC/DEC/(06)01 [6], *on the harmonised utilisation of spectrum for terrestrial IMT-2000/UMTS systems operating within the bands 1900-1980 MHz, 2010-2025 MHz and 2110-2170 MHz*, came into force, aiming at facilitating efficiency in utilisation of the IMT-2000/UMTS bands across CEPT by identifying a common approach to spectrum planning. It entered initially into force on 24 March 2006 and addressed both paired (1920-1980 MHz and 2110-2170 MHz) and unpaired (1900-1920 MHz and 2010-2025 MHz) frequency bands. In addition, it replaced the earlier Decisions ERC/DEC/(97)07 [5], ERC/DEC/(99)25 [3] and ERC/DEC/(00)01 [4], consolidating and updating their provisions, removing references to self-provided applications operating in self coordinating mode, and allowing flexibility between FDD uplink and TDD modes of operation in the bands 1900-1920 MHz and 2010-2025 MHz. The values used in Annex 1 of Decision ECC/DEC/(06)01 [6] have been based on the inter-service compatibility studies from ERC Report 65 [13], and intra-service carrier spacing studies undertaken within ETSI SMG02.

ECC conducted in 2010-2011 a review of this ECC/DEC/(06)01 [6] taking into account the information on the practical implementation and authorisations in force. During the revision process, CEPT came to the conclusion that the unpaired 2 GHz bands were mostly unused and there was absence of equipment from manufacturers; the band 1900-1920 MHz, although licensed in many countries, remained largely unused, and the use of frequencies in the band 2010-2025 MHz had only been authorised in few countries. Frequency arrangements for the unpaired 2 GHz bands have been removed from the revision of ECC/DEC/(06)01 [6] and it was concluded that further investigations are needed to develop a suitable ECC framework for those bands.

The European Common Allocations Table (ECA) [14] of frequency allocations and applications in the frequency range 8.3 kHz to 3000 GHz in its latest version from March 2013 includes for the bands 1900-1930 MHz and 2010-2025 MHz the MOBILE service and the Fixed service (secondary status in the ECA). The ECA already indicates that CEPT is investigating alternative usage for the unpaired 2 GHz bands.

## Current authorisations and uses of the unpaired 2 GHz bands

Currently, all or parts of the frequency band 1900-1920 MHz is licensed to mobile operators for the provision of electronic communications services in 36 CEPT countries, whereby the licences are mainly limited to UMTS/IMT-2000 TDD technology. On the other hand, the frequency band 2010-2025 MHz, or parts of it, is licensed to mobile operators in 13 CEPT countries for the provision of electronic communications services, mainly limited to UMTS/IMT-2000 TDD technology and in some cases in a technology-neutral way. Existing licences in the unpaired 2 GHz bands have been awarded on an exclusive basis in some countries. In addition, some administrations use the band 2010-2025 MHz for short term licences, in particular for wireless cameras. Annex 3 shows the current authorisations in the bands 1900-1920 MHz and 2010-2025 MHz and the corresponding duration.

The mobile licences (UMTS TDD) in force on the unpaired 2 GHz bands are not in use in Europe, noting also that the lack of interest of mobile operators for spectrum in the unpaired terrestrial 2 GHz band has been demonstrated during the auctions in some CEPT countries in 2011. The duration of those licences vary from country to country, from 2014 - 2029 (or even unlimited duration, in United Kingdom).In addition it has to be mentioned that some licences have already been surrendered in a number of countries.

Some of the licences were awarded after spectrum auction processes and, as a result, considerable auction prices were achieved. In some countries, a licence repeal process might be possible in case of continued non-implementation, whereas in other countries this will not be possible due to specific conditions and obligations which are part of the licence (e.g., coverage obligations are interpreted in some cases as fulfilled when providing services via other spectrum where the same licensee has also a licence and for which the network is implemented).

Other options for making the spectrum available for new usage need to be considered (e.g. liberalisation, transfer, interim licence conditions for new licensee until the end of the existing licence duration(s)). Liberalisation frameworks would permit incumbent licensees in many of these countries to enable alternative service deployment, but the frameworks in some countries would or may maintain restrictions with regard to technology or use. A number of administrations may not be in a position to withdraw the existing licences and may seek agreements between the existing licence holder and possible new service operator(s). According to the results of a CEPT questionnaire on authorisation issues regarding the candidate bands for Broadband Direct-Air-to-Ground Communications (DA2GC) in 2013, the prospects for change of use through liberalisation appear in general promising for the 2 GHz unpaired bands, whereby the precise liberalisation framework may need to be found by the individual administration. It may be helpful to describe more in detail the options for a precise liberalisation framework in accordance with the needs of the new foreseen spectrum usages (e.g. pan-European service coverage in case of DA2GC) and to set up a common European implementation schedule for future harmonised and efficient use of the 2 GHz unpaired bands. The difficulties related to current regulations and possible options for a liberalisation framework will be described in the Final Report from CEPT, which will detail the work undertaken and present final results under this Mandate.

Updated information on the current status of individual authorisations in force on the unpaired 2 GHz bands can be found in ECO Report 003 [9] (<http://www.cept.org/eco/deliverables/eco-reports>) and EFIS (<http://www.efis.dk/>).

## Current use and regulatory framework outside CEPT

The following information has been collected on the current use and regulatory framework outside of CEPT as shown in Table 1.

Table 1: Current Use and Regulatory Framework in Countries outside of the CEPT

|  | **1900-1920** | **2010-2025** |
| --- | --- | --- |
| **Australia** | Mobile telephony – licence expiry 2017  Capital cities only—3G and BWA services.  Regional and remote areas only—BWA.  Review initiated. | Mobile telephony – licence expiry 2017  Capital cities only—3G and BWA services.  Regional and remote areas only—BWA.  Review initiated. |
| **Canada** | 1 850 - 2 000  FIXED  MOBILE 5.384A 5.388A  5.388 5.389B C35:  In the band 1 850-1 990 MHz, stations of the mobile service have priority over those of the fixed service with displacement of fixed assignments governed by the appropriate spectrum utilization policy. | 2 020 - 2 025  FIXED  MOBILE  5.388 C37:  The designation of the band  2 020-2 025 MHz for Advanced Wireless Services may be the subject of a future public consultation. |
| **China** | 1900 – 1915 MHz is planned to be allocated to Digital Low Tier cordless telephony. Deployment of both private cordless telephones and wireless local loop based on DECT is anticipated, in the band 1900-1920 MHz allocated by the Office of State Radio Regulatory Commission, OSRRC. The OSRRC has decided that only TDD radio technologies may operate within this band, but beyond this the Chinese regulator is not being technology specific. Thus other TDD technologies, notably PHS, will be allowed to be used within this allocation.  1895 - 1905 MHz can be also allocated to the third generation (3G）mobile telecommunications service.  1915 - 1975MHz are allocated to the third generation（3G）mobile telecommunications service. | IMT-2000 services（WRC-2000）  1885 - 1980, 2010 - 2025 MHz can be allocated to the IMT-2000 high altitude platform stations (HAPS) service (WRC-2000）  2010 – 2025 MHz are allocated to the third generation（3G）mobile telecommunications service. |
| **CITEL** | DECT usage is allowed in many countries administered by CITEL, within the frequency band 1910-1930 MHz allocated in:  Argentina  Bahamas  Bolivia  Brazil  Chile  Colombia  Costa Rica  Dominican Republic  El Salvador  Equador  Honduras  Mexico  Panama  Paraguay  Peru  Uruguay |  |
| **Africa CRASA**  **CRASA groups together the 14 Southern African Development Community (SADC) countries** | 1 900-1 920 MHz  FWA  IMT (terrestrial) | IMT (terrestrial) (2010-2025 MHz)  TDD |
| **India** | 1900-1910 MHz paired with 1980-1990 MHz may be considered for cellular systems | 2010-2025 MHz (TDD mode) |
| **Japan** | 1885-1980 MHz  J99  FIXED  Commercial Telecommunications Service (Fixed Wireless Access Communications in 1900MHz)  The band 1885-2025MHz is intended for use by IMT-2000. Such use does not preclude the use of these bands by other services to which they are allocated (see also PHS- Personal Handyphone System – a cordless telephony system)  The band 1893 – 1906 MHz is used by DECT in Japan (sharing the band with PHS) | 2010-2025 J99  MOBILE J99A J99B  Commercial Telecommunications Service (Portable Radio Communications)  An assignment to the Portable Radio Communications is subject to Annex 7-3.  The bands 1885-1980MHz, 2010-2025MHz may be used by high altitude platform stations as base stations to provide IMT-2000. |
| **United States** | 1850-2000  FIXED  MOBILE  RF Devices (Part 15)  Personal Communications (Part 24)  Fixed Microwave (Part 101)  1980-2010 MHz  NG177  NG177 In the bands 1990-2000 MHz and 2020-2025 MHz, where the receipt date of the initial application for facilities in the fixed and mobile services was prior to June 27, 2000, said facilities shall operate on a primary basis and all later-applied-for facilities shall operate on a secondary basis to any service licensed pursuant to the allocation adopted in FCC 03-16, 68 FR 11986, March 13, 2003 (“Advanced Wireless Services”). Not later than December 9, 2013, all such facilities in the bands 1990-2000 MHz and 2020-2025 MHz shall operate on a secondary basis to Advanced Wireless Services. | 2000-2020 MHz  FIXED  MOBILE  MOBILE-SATELLITE  (Earth-to-space)  Satellite Communications (Part 25)  2020-2025 MHz  FIXED  MOBILE  NG177 |

From Figure 1 it can be concluded that there is an extensive use by PHS services outside of Europe.




Figure 1: PHS Deployment

Table 2: Frequency bands usable for PHS

|  |  |
| --- | --- |
| Country/Area | Frequency Band |
| Asia | |
| Bangladesh | 1895.0 - 1915.0 |
| China | 1900.0 - 1920.0 |
| India | 1880.0 - 1900.0 |
| Indonesia | 1895.0 - 1918.1 |
| Japan | 1884.5 - 1919.6 |
| Philippines | 1908.0 - 1918.0 |
| Singapore | 1895.0 - 1906.1 |
| Taiwan | 1905.0 - 1915.0 |
| Thailand | 1900.0 - 1918.1 |
| Vietnam | 1895.0 - 1900.0 |
| Pacific | |
| Australia | 1880.0 - 1900.0 |
| New Zealand | 1895 - 1920 |
| Middle East & Africa | |
| Cameroon | 1905.0 - 1920.0 |
| Ethiopia | 1905.0 - 1925.0 |
| Mali | 1885.0 - 1930.0 |
| Swaziland | 1895.0 - 1905.2 |
| U. A. E. | 1895.0 - 1905.0 |
| North America | |
| USA | 1880.0 - 1910.0 1915.0 -1920.0 |
| Latin America | |
| Argentina | 1880.0 - 1910.0(mobile) 1910.0 - 1930.0(fixed) |
| Brazil | 1880.0 - 1900.0 |
| Chile | 1880.0 - 1910.0(mobile) 1910.0 - 1930.0(fixed) |
| Columbia | 1880.0 - 1910.0(mobile) 1910.0 - 1930.0(fixed) |
| Costa Rica (Fixed) | 1910.0 - 1930.0(fixed) |
| Guatemala | 1910.0 - 1918.0 |
| Haiti | 1910.0-1930.0 |
| Honduras (Mobile) | 1880.0 - 1910.0(mobile) 1910.0 - 1930.0(fixed) |
| Uruguay | 1910.0 - 1930.0 |

PHS services range from digital walky-talky to cordless telephony, WLL and local FWA (up to about 10 km distance), private as well as public PHS services.

<http://www.phsmou.org/resources/PHSGuidebook_4th.pdf>

By October 2006, the PHS service had as many as 93 million subscribers in about 600 cities in China. The public PHS service in Taiwan is estimated to have at least 2 million subscribers.

## Previous studies on the unpaired 2 GHz bands

CEPT Report 039 [11] has been the most recent work on the Unpaired 2 GHz frequency bands. This CEPT Report 039 [11] was built on the work carried out in ERC Report 065 [13], by considering developments in characteristics of systems operating in adjacent bands and by considering technology-neutral approach to allow technologies other than UMTS to be deployed. It was found that the conclusions of ERC Report 065 remain valid. CEPT Report 039 [11] was prepared by CEPT in response to the Mandate from the European Commission, issued in June 2009, relating to the 2 GHz bands (1900-1980/2010-2025/2110-2170 MHz).

Available studies identified are ERC Report 064 [12] (Sharing between UMTS and existing fixed services) and ERC Report 065 [13] (Adjacent band compatibility between UMTS and other 2 GHz services), both addressing the bands 1900-1920 MHz and 2010-2025 MHz. These reports have been agreed in 1999 in the context of the designation of the bands for UMTS.

In addition, CEPT Report 019 [10] was prepared in response to the EC Mandate to develop least restrictive technical conditions for frequency bands addressed in the context of WAPECS. The Final Report was issued on 21 December 2007, with editorial revisions made on 17 March 2008 and 30 October 2008.

## Identification of alternative uses for both unpaired 2 GHz bands

CEPT had investigated, in the past three years before the EC Mandate was issued, many usage scenarios for the frequency bands 1900-1920 MHz and 2010-2025 MHz, in view of finding a suitable solution for the currently unused unpaired 2 GHz bands. The following options were considered and duly investigated:

* the pairing of 1900-1920 MHz and 2010-2025 MHz (between themselves or with others frequency bands) for IMT;
* the potential use of the unpaired band by low power applications;
* the identification of alternative uses for 1900-1920 MHz and 2010-2025 MHz bands.

As a result of a detailed analysis conducted within CEPT, the following alternative uses for the unpaired 2 GHz bands were considered the most suitable solutions as a result of the CEPT investigation:

1. Use (parts of) the bands 1900-1920 MHz and/or 2010-2025 MHz to satisfy the spectrum demand of 20 MHz TDD or 2x10 MHz FDD for **Broadband DA2GC**.

The following options / combinations of bands for Broadband DA2GC would be possible:

* Use of the band 1900-1920 MHz for **TDD Broadband DA2GC** (guard bands may be required);
* Pair 10 MHz within the band 1900-1920 MHz with 10 MHz within the band 2010-2025 MHz for FDD Broadband DA2GC (guard bands may be required), as follows:



Figure 2: Spectrum map considering FDD BDA2GC

and

use the remaining 15 MHz within 1900-1920 MHz and 2020-2025 MHz for **video links and/or other SRDs** (guard bands may be required);

* Pairing of the bands 1900-1920 MHz and 2010-2025 MHz, from a cellular mobile point of view (mass market), was studied. Increased complexity (additional bands) in User Equipment (UE) design compared to very limited economic benefits for the cellular mobile community led to lack of support from Industry. The situation was considered different for Broadband DA2GC, due to equipment dedicated to these two bands only;

1. Use of the entire 1900-1920 MHz and/or 2010-2025 MHz band for **PMSE** (in particular, video links); **several PMSE use cases have been identified;**
2. Use of both bands for **SRDs** (e.g.: among those applications requiring spectrum in the 2.4 GHz band); it has been noted that studies would first require the knowledge and identification of the future primary service use(s) in the bands;
3. To make spectrum in the band 1900-1920 MHz available for DECT, which is adjacent to the 1880-1900 MHz band (the “DECT” band)..
4. **Ad-hoc** **Broadband PPDR** network (potential compatibility to be confirmed); some use cases could be technically identical with identified PMSE use cases such as for wireless camera usage.

Any of the above alternative uses for the unpaired 2 GHz spectrum were considered to need further assessment in view of identifying the corresponding relevant technical conditions.

The future use of the unpaired 2 GHz bands could, in some cases, be considered on a band sharing basis (depending on the applications to be considered, geographical separation ought to be required to avoid interference).

It was as well be noted that harmonisation in the short term could be hampered by the individual authorisations in force in some countries.

# ALTERNATIVE USES INCLUDING SPECTRUM REQUIREMENTS

In order to respond to the request of the EC mandate, the following alternative uses are considered under this section:

1. Broadband Direct Air to Ground Communications;
2. Programme Making and Special Events;
3. Short Range Devices *;*
4. Digital Enhanced Cordless Telecommunications;
5. Public Protection and Disaster Relief.

It should also be noted that for these radio applications frequency bands other than the unpaired 2 GHz bands are also under consideration or have already been designated on CEPT level.

As described in section 3.6, synergies are identified so far for PMSE and ad hoc PPDR usages (use of the same technical framework and equipment) as well as for DECT and SRD usages (both candidates are seeking an allocation under a general authorisation regime). There may be a possibility of having a common set of technical parameters to enable equitable spectrum access.

## Broadband Direct Air to Ground Communications

Several ECC Reports are currently under development within CEPT/ECC describing frequency management related and compatibility/sharing issues, see also section 4: the draft ECC Report on Broadband Direct-Air-to-Ground Communications (DA2GC) [26], ECC Report 209 on compatibility/sharing studies related to Broadband Direct-Air-to-Ground Communications (DA2GC) in the frequency bands 1900-1920 MHz / 2010-2025 MHz and services/applications in the adjacent bands [27] and the draft ECC Report on Compatibility between DA2GC and PMSE video links in the 2 GHz unpaired bands [29].

Additionally, because other frequency bands - especially 5855-5875 MHz - have also been studied for Broadband DA2GC, ECC Report 210 on Compatibility/sharing studies related to Broadband Direct-Air-to-Ground Communications (DA2GC) in the frequency bands 5855-5875 MHz, 2400-2483.5 MHz and 3400-3600 MHz [28] has been developed.

### Introduction

A Broadband DA2GC system constitutes an application for various types of telecommunications services, such as internet access and mobile multimedia services. It aims to provide access to broadband communication services during continental flights on a Europe-wide basis. The request for spectrum is related to the direct-air-to-ground radio solution. The connection with the flight passengers’ user terminals on-board aircraft is to be realised by already available fixed or Wi-Fi-based on-board connectivity network and/or via GSMOBA and in the future possibly also via UMTS and/or LTE.

The main application field would be Air Passenger Communications (APC). In addition a Broadband DA2GC system could also support Airline Administrative Communications services (AAC) and thus improving aircraft operation, resulting in particular in reduced OPEX for the airlines. Safety-relevant communications such as Air Traffic Control (ATC) and related services are not intended to be covered.

European Airlines are following the CEPT activities on Broadband DA2GC. So far Lufthansa / Swiss / Austrian airlines, KLM / Air France, Air Berlin and British Airways have sent letters to CEPT showing their interest in a solution for Broadband DA2GC in Europe.

European companies represent an important force in the aeronautical market. The European aircraft industry holds about 50% of the world market for aircraft manufacturing. In the field of Air Passenger Communications services, however, Europe has room for improvements when compared to other parts of the world.

In North America an air–to-ground system has been established in the duplex bands 849-851 MHz and 894-896 MHz, since the year 2008, with more than 2 000 commercial aircraft and 5 000 business aircraft equipped so far. An extension of the spectrum in the order of 2x1 MHz is going to be realised in the near future. In addition, the FCC is considering a new proposed rulemaking for DA2G Communications at 14.0-14.5 GHz (sharing with the FSS uplink whereby DA2GC ground stations avoid transmissions into the geostationary arc).

China is currently testing CDMA EV-DO to cover all of China's air routes. The industry is also studying the use of the fourth-generation mobile communications standard LTE, which provides higher download speeds, for route coverage. Trials for DA2G communications are underway under the direction of CAA China and other Chinese Government entities to operate in 1785-1805 MHz band (20 MHz total bandwidth for DA2GC) and using TD-LTE technology. At present, China Telecom has constructed four surface-to-air base stations on the Beijing-Chengdu route, and has a total of 17 base stations completed as of early 2012. Under the plan, China will construct up to a thousand surface-to-air base stations in the next few years. China's Civil Aviation Air-Ground Broadband Communications System will cover all routes of the major domestic airlines.

For the purpose of the present document the following definitions apply:

Table 3: Definitions for Broadband DA2GC

| **Term** | **Definition** |
| --- | --- |
| Aircraft Station (AS) | Entity on-board aircraft providing the radio, control and telecommunication functionalities for broadband DA2G communication. |
| Direct-Air-to-Ground Communications | Direct radio link between an Aircraft Station (AS) and a Ground Station (GS). |
| Forward Link (FL) | Within the DA2GC system the link from the Ground Station (GS) to the Aircraft Station (AS). |
| Ground Station (GS) | Entity on the ground providing the radio, control and telecommunication functionalities for DA2GC. |
| Reverse Link (RL) | Within the DA2GC system the link from the Aircraft Station (AS) to the Ground Station (GS). |

### Motivation for Broadband DA2GC

Mobile customers expect to be connected everywhere, every time, with all kind of mobile devices. This includes the provision of broadband services on-board aircraft and European airlines have great interest to offer internet services to their flight passengers in their continental fleets as soon as possible.

The connection link between the aircraft and the ground can be established either via satellites or by means of Direct-Air-to-Ground Communications (DA2GC). For future broadband services, it can be foreseen that the service provision via satellite will be conducted by using Ka-band satellite capacity and a considerable number of Ka-Band satellites are already put into operation or under procurement. Satellite operators also consider mobile platforms such as aircraft and vessels as a considerable part of the addressable market and the ECC has recently adopted and published new ECC/DEC/(13)01 [7] supporting Earth Stations on Mobile Platforms (ESOMP). Ka-band satellite as well as DA2GC can therefore be seen as technical solutions in competition. On the other side, both solutions could also complement each other.

The establishment of a pan-European regulatory environment for Broadband DA2GC would provide ample benefits for the users - i.e. airline companies and flight passengers - in Europe:

* As an alternative service provision which by fostering competition might lead to a lower cost for the airlines and for the flight passengers;
* The technical implementation of DA2GC and also the stimulus of competition may lead to a provision of services at improved cost structures - including non-safety-relevant administrative communication services - and hence create a benefit to end customers and airlines resulting in higher and earlier service take-up;
* DA2GC avoids the round trip delay that is typical and unavoidable for geostationary satellite service provision and hence can provide low latency services;
* The costs for aircraft installations and maintenance are a key issue for airline companies. Given the fact the DA2GC equipment can be installed overnight to a plane is seen as an advantage by airline operators. In particular with regard to the aircraft antenna, a terrestrial solution has a clear advantage compared to existing satellite usage.

A further motivation arises from the expected growth of the air traffic. A forecast from Eurocontrol[[1]](#footnote-1) published in October 2011 estimates 11.5 million movements under Instrument Flight Rules (IFR) in Europe in 2017. This is 21% more than in 2010.

About 66% of the European air traffic consists of domestic or continental flights, i.e. the main part of the airline business. The addressable market in Europe for DA2GC is currently consisting of about 160 airlines with more than 4500 aircraft expected in 2014 (without business aviation). In general a strong increase in percentage of aircraft fleet equipped with internet connectivity solutions is expected during the next years. According to a market research[[2]](#footnote-2), approximately 50% of the world’s fleet will have been equipped with Wi-Fi connectivity by 2020.

The introduction of Broadband DA2GC would not only increase Europe’s competitive position, but it could also bring Europe into a leading position in this market segment. Studies on air passenger demand for on-board connectivity are currently not publicly available.

The introduction of Broadband DA2GC providing mobile services would contribute to the development of the internal market and enhance competition by increasing the availability of pan-European services and end-to-end connectivity as well as encouraging efficient investment. DA2GC constitutes an innovative alternative platform for various types of pan-European telecommunications services provided to aircraft passengers.

The provision of broadband services including also all kinds of transportation sectors is a declared goal under the European Digital Agenda 2020 plans.

Broadband DA2GC provide such services without the round trip delay that is a feature in the competing geostationary satellite service solutions. In addition, these networks can provide services to airplanes by using aircraft antennas that are considerably efficient in terms of weight, size, aircraft installation costs and air drag considerations when compared to satellite antennas on-board aircraft.

### Spectrum Demand for Broadband DA2GC

The spectrum demand for Broadband DA2GC is derived from a summary of relevant factors to be essential to cope with future capacity demand as well as from results achieved by system performance evaluations.

Statistical traffic evaluations show that there is an average number of more than 26 aircraft simultaneously within one cell with coverage radius of 100 km in high air traffic areas which are concentrated in Western/Central Europe (mainly Germany, France, Benelux, Switzerland, Austria, United Kingdom, Northern Spain and Northern Italy). It has to be mentioned that there are also areas at the edge of the flight zones, where the cells have only a low traffic density in the range of 1 - 2 aircraft simultaneously, but the spectrum demand for Broadband DA2GC has to be adapted for the high traffic areas. The approach used assumes that about 60% of the fleets are covered.

Based on the calculations which have been carried out and accepted so far within ECC, paired spectrum of 2x10 MHz for FDD operation is agreed to be necessary to cope with short- to medium-term demand. Unpaired spectrum for TDD operation (up to 20 MHz) would also be an option. The amount of spectrum released could be done on a step-by-step process, e.g. by allocating the spectrum in smaller blocks on a national basis. This could be a methodology for facilitating a time plan for a common European harmonisation.

A future spectrum designation for Broadband DA2GC should be technology-neutral as far as possible by taking into account the three different system descriptions as developed by ETSI (TR 103 054 [31], TR 101 599 [32] and TR 103 108 [33]).

The implementation and operation of more than one European Broadband DA2GC system in the same frequency band (either in the unpaired 2 GHz bands or on the 5.8 GHz band) was considered as unlikely. Therefore intra-service sharing studies (e.g. for 2 Broadband DA2GC systems in the unpaired 2 GHz bands) were not carried out. However, by looking at the results of the compatibility and sharing studies it appears that co-channel operation of different Broadband DA2GC systems would not be possible in the same geographical area. Even in the case of different systems in adjacent frequency blocks (in the same geographical area) a guard block in between seems to be necessary if TDD is considered. No aggregate effect with regard to other radio applications, i.e. adjacent to the unpaired 2 GHz bands, may occur.

As mentioned earlier, the roll-out of a European wide Broadband DA2GC system may be facilitated by releasing the spectrum using a step by step process. Cross-border coordination amongst European countries is considered to be an issue that can be addressed with normal bilateral/multilateral coordination procedures. In addition, it is considered that there will be no legacy systems (i.e. UMTS/TDD) in operation to coordinate with. Coordination with services within bands (e.g. PMSE) or in adjacent bands - either within a country or between neighbouring countries - is expected to be based on the results of the compatibility studies.

The results of the compatibility and sharing studies provide also a basis for cross-border coordination at the outer European borders, such as separation distances between DA2GC GS and other radio stations in the neighbouring country or for appropriate measures for the AS (e.g. power reduction over relevant countries without a DA2GC service). Although the situation - i.e. non-utilisation of the spectrum - outside of CEPT in ITU Region 1 is most likely similar because of the current IMT identification of the unpaired 2 GHz bands, such coordination would also support that a pan-European DA2GC service would not be subject to operational restrictions at border areas in the future.

### Compatibility/sharing scenarios for DA2GC in the 2 GHz unpaired bands

A number of different compatibility/sharing scenarios with other radio services/applications were considered for the implementation of DA2GC within the 2 GHz unpaired bands. In addition, the possibility to put the DA2GC FL as well as the DA2GC RL within either band were also subject for the studies. All these compatibility/sharing scenarios are illustrated in Figure 3 to Figure 6.



Figure 3: Compatibility/sharing scenarios for BDA2GC RL in the frequency band 1900-1920 MHz

Compatibility_Scenarions_DA2G_FL_1900-1920MHz

Figure 4: Compatibility/sharing scenarios for BDA2GC FL in the frequency band 1900-1920 MHz

Beschreibung: Compatibility_Scenarions_DA2G_RL_2010-2025MHz

Figure 5: Compatibility/sharing scenarios for DA2GC RL in the frequency band 2010-2025 MHz



Figure 6: Compatibility/sharing scenarios for DA2GC FL in the frequency band 2010-2025 MHz

The following three options would appear to be the preferred ones as a result of the compatibility studies between Broadband DA2GC and existing services adjacent to the unpaired 2 GHz bands:

* For an FDD system according to ETSI TR 103 054, frequency bands: 1900-1910 MHz  
  (FL) and 2010-2020 MHz (RL).
* For a TDD system according to ETSI TR 101 599, frequency band: 1900-1920 MHz.
* For a TDD system according to ETSI TR 103 108, frequency band: 1900-1920 MHz.

It should be noted that the two TDD options mentioned above are also under consideration for Broadband DA2GC in the 5.855-5.875 GHz band.For the time being the possibilities for a TDD system in the frequency band 2010-2025 MHz will not further be considered. This is due to a decision taken at a previous WG FM meeting. During the Call for Inputs, no preference for a TDD solution in the 2010-2025 MHz band has been indicated by any responder. The 2010-2025 MHz band can only provide up to 15 MHz for DA2GCS using TDD, although it is seen as technically possible to operate such a system also within less than 20 MHz. However, as long as not all results on the on-going compatibility and sharing studies are available (especially the results regarding sharing with PMSE and other candidate applications as mentioned in the mandate) no other option should be completely excluded.TDD within 2010-2025 MHz might be revisited in the future or a technologically neutral approach enabling either FDD or TDD usage within 1900-1910 MHz and 2010-2020 MHz.

## Programme Making and Special Events

The term Programme Making[[3]](#footnote-3) and Special Events[[4]](#footnote-4) applications (PMSE) describes radio applications used for SAP/SAB, ENG/OB and applications used in meetings, conferences, cultural and education activities, trade fairs, local entertainment, sport, religious and other public or private events for perceived real-time presentation of audiovisual information.

The definitions of SAP/SAB and ENG/OB are set out[[5]](#footnote-5) as follows:

**SAP:** Services Ancillary to Programme making (SAP) support the activities carried out in the making of “programmes”, such as film making, advertisements, corporate videos, concerts, theatre and similar activities not initially meant for broadcasting to general public.

**SAB:** Services Ancillary to Broadcasting (SAB) support the activities of broadcasting industry carried out in the production of their programme material.

The definitions of SAP and SAB are not necessarily mutually exclusive. Therefore they are often used together as “SAP/SAB” to refer generally to the whole variety of services to transmit sound and video material over the radio links.

**ENG:** Electronic News Gathering (ENG) is the collection of video and/or sound material by means of small, often hand-held wireless cameras and/or microphones with radio links to the news room and/or to the portable tape or other recorders.

**OB:** Outside broadcasting (OB) is the temporary provision of programme making facilities at the location of on-going news, sport or other events, lasting from a few hours to several weeks. Mobile and/or portable radio links are required for wireless cameras or microphones at the OB location. Additionally, radio links may be required for temporary point to point connections between the OB vehicle, additional locations around it, and the studio.

The definitions of ENG and OB are not mutually exclusive and certain operations could equally well reside in either or both categories. Therefore, it has been a long practice within the CEPT to consider all types of such operations under the combined term “ENG/OB”. It is also understood that ENG/OB refers to terrestrial radiocommunication services, as opposed to SNG/OB term, which refers to similar applications but over the satellite radiocommunication channels.

PMSE covers a wide variety of applications. Those most suitable for the unpaired 2 GHz bands consist of wireless cameras and mobile video links. Typically these services are allocated spectrum in blocks of 10 MHz bandwidth. The neighbouring band 2025-2110 MHz is already used in at least 19 CEPT countries for such PMSE applications on a shared basis, and is identified on a tuning range basis in ERC/REC 25-10 [17] (relevant extracts presented in ANNEX 3:). The term “tuning range” for PMSE refers to a range of frequencies over which radio equipment is envisaged to be capable of operating. In any given country none, some or all of the tuning range may be available for assignment for PMSE use, usually on a geographically-, frequency-, power- and time-limited basis. The availability of spectrum for PMSE use is dependent on the sharing conditions with the primary users of the spectrum at any given location.

The successful use of video PMSE (as with other radio services) is dependent upon a range of factors which contribute to the link budget. The 2-3 GHz range provides the best conditions for many applications, including airborne and mobile use. The physical size of 2 GHz antennas and the attractive propagation characteristics, including using reflections from surrounding objects, allow successful capture of high quality images for mobile use, for example a camera operator running along the touchlines at a football match, or sitting on a motorbike following a road race. This frequency range is effective even in partially obstructed propagation paths, such as ground to air links obstructed by trees.

Due to a number of changes to the allocation of spectrum in the 2-3 GHz range, this frequency range is becoming more limited for use by PMSE. ERC/REC 25-10 [17] identifies 575 MHz of spectrum in the   
2-3 GHz range (2025-2110 MHz, 2200-2690 MHz) as tuning range for PMSE. However, recent allocations to services with which PMSE cannot share (e.g. in the 2.5-2.69 GHz band and potentially within the 2.3-2.4 GHz band depending on future studies within CEPT) has resulted in a significant reduction of available spectrum for PMSE. The requirements for spectrum in the 2-3 GHz range remains, and with the advent of increased HD and UHD production, additional requirements may be foreseen. Several candidate bands within an extended tuning range for possible future use for cordless cameras and video links are under consideration (CEPT Report 51).

The 2010-2025 MHz band is directly adjacent to the 2025-2110 MHz band that is already part of the tuning range for video PMSE applications. Commonly, video PMSE equipment is already capable of tuning to this range; indeed, in some CEPT administrations, this band is already used on a temporary basis for PMSE. For the 1900-1920 MHz band, however, equipment is generally not able to tune and modifications would be required to existing and future equipment. As such, the 2010-2025 MHz band has a higher immediate potential for wider use within CEPT countries for video PMSE than the 1900-1920 MHz band.

Video PMSE is used in a wide variety of programme production and film making, from daily news events with a single camera, through sporting events such as football which typically uses two or three wireless cameras, to more major productions, both studio based and outdoor which may require many cameras, mobile and airborne links to produce.




Figure 7: Cordless Camera for Sports Coverage

The typical technical characteristics of wireless video PMSE applications are given in table 1 of ERC Report 38 [19] (relevant extracts presented in **Error! Reference source not found.**).

## Short Range Devices

Based on the requests from ETSI set out in five ETSI system reference documents for SRD applications, CEPT developed ECC Report 189 [30] on future spectrum demand for Short Range Devices in the UHF frequency bands 870-876/ 915-921 MHz. This includes spectrum demands raised by ETSI for generic SRD, UHF RFID, Home Automation & Sub Metering, automotive SRD, Smart Meters and Smart Grids, Metropolitan Mesh Machine Networks (M3N) applications, Alarm and Social Alarm systems and Assistive Listening Devices. At the same time, no demand request has been received for the unpaired 2 GHz band.

The propagation characteristics of 2 GHz is not as good for many applications, e.g. smart metering/ smart grids, compared with the spectrum considered in the on-going investigations under the UHF roadmap for which five ETSI System Reference Documents had been received, expressing proposals for utilizing the 870-876 MHz and 915-921 MHz frequency bands. It can be concluded from investigations that frequencies around 2 GHz are sub-optimal for installations in basements in urban and suburban areas (e.g. only around 20% of all smart meters could be reached according to an extensive study presented to SRD/MG by the University of Dortmund which was commissioned by German authorities). The UK Department of Energy and Climate Change also provided statements in support of a solution below 1 GHz as under the on-going investigations.

On the other side, examples where 2 GHz can be used are e.g. industrial automation, some alarm systems, machine-to-machine. For industrial automation applications, CEPT is currently investigating also the 5725-5875 MHz frequency range.

A 2 GHz solution would also be limited to Europe only since existing usages outside of Europe do not foresee SRD applications in the 2 GHz unpaired bands and many SRD applications such as RFID or wireless applications in industry were looking for frequency opportunities which could also be used in other regions. The prospects for global harmonisation in the 800/900 MHz look better due to the presence of the 902-928 MHz ISM-band in Region 2 and this aspect is very important for some market sectors such wireless solutions used at machines, aircraft, automotive, RFID.

In addition, it should be noted that the particularity of SRD application is that none allocation are required to operate in a frequency band. This means that a simple request from industry would be taken into account at any time but preferably when a primary user will be identified.

Regarding the proposal for DECT as set out in section 3.4, if this is realised under application-neutral and technology-neutral principles (see CEPT Report 014 [1] and CEPT Report 044 [2]) using general authorisation, it can also be regarded as a new spectrum opportunity for SRD usage, provided that suitable spectrum access rules are followed (see section 3.6 on Synergies between the proposed short list of selected use). The DECT proposal and the SRD approach are identical with regard to equal and non-exclusive access to spectrum under exemption from individual authorisation, in a spectrum compatible way with other possible usage which could be under individual authorisations, e.g. a DA2GC ground network.

Apart from the DECT system reference document, there is no ETSI system reference document under preparation in ETSI at the moment nor an industry request for SRD applications, making a proposal for usage in the 2 GHz Unpaired bands. The technical parameters of the DECT system reference document are proposed to be used for compatibility studies. CEPT is aware of other technologies with similar technical parameters and spectrum access mechanism, e.g. IEEE 802.11ah (both approaches with 250 mW e.i.r.p., 1 MHz channel bandwidth, dynamic channel/frequency selection spectrum access mechanism). The proponents of the technology 802.11ah have approached the CEPT with the request for identifying a spectrum opportunity for sub-1 GHz frequencies.

CEPT recommends that the principles set out in CEPT Reports 14 and 44 for technology-neutral and application-neutral license-exempt regulations should apply for the DECT proposal. This does however not ensure that other standards will be developed with similar (or equivalent) medium access mechanism, and able to compete with DECT in the same spectrum.

A proposal to consider metering (smart metering, smart grids and smart cities) in the unpaired bands was presented during the Call for Inputs, taking note that the needed frequency ranges are dependent on a country’s geography and the average construction of houses and buildings. It is as well referred that a number of bands proposed for metering, such as the 870-876 MHz, are not available in a substantial number of countries.

In line with the SRD strategy set out in CEPT Reports 14, 43 and 44 for metering applications, as well as the recent RSPG Report on Sectoral Needs, metering devices should be covered by a non-specific SRD regulatory approach. This request is therefore already included in the DECT/SRD usage block (see section 3.6).

## Digital Enhanced Cordless Telecommunications

Digital Enhanced Cordless Telecommunications (DECT) is a general radio access technology for wireless telecommunications, for cell radii ranging from a few meters to several kilometers, depending on application and environment. The DECT technology provides a comprehensive set of protocols which provide the flexibility to interwork between numerous different applications and networks. The base standard EN 300 175-1 to 8 [16] specifies a high capacity TDMA/TDD radio interface supporting symmetric and asymmetric connections, connection oriented and connectionless data transport and provides security and confidentiality services. The mandatory instant Dynamic Channel Selection (iDCS) messages and procedures provide effective co-existence of uncoordinated private and public systems on the common designated DECT frequency band and avoid any need for traditional frequency planning.

In 1989, CEPT agreed Recommendation T/R 22-02 [20] which designated the band 1880-1900 MHz for DECT (abrogated in the meantime). In 1991, Council of the European Communities adopted a Directive[[6]](#footnote-6) which required member states to designate 1880-1900 MHz for DECT and to ensure that any services remaining in this band do not interfere with any DECT systems that may be established according to commercial demand. CEPT developed then two decisions on DECT;

* ERC/DEC/(94)03 [21] on the frequency band to be designated for the coordinated introduction of the Digital European Cordless Telecommunications system;
* ERC/DEC/(98)22 [22] on Exemption from Individual Licensing of DECT equipment, except fixed parts which provide for public access (Amended 8 November 2013).

The current regulation does not restrict the scope of DECT applications (e.g., audio, video).

### Reasons for proposing additional spectrum for DECT

DECT technology has over 820 million of accumulated devices since its introduction in the market. The accumulated number of DECT devices grows at a ratio of around 100 M devices per year. This is far more than initially expected and is supported by only 20 MHz of allocation. While the operation of the technology is currently successful, it appears prudent to assign additional bandwidth for further expansion of the technology.

DECT was initially primary a 3.1 kHz telephony service conveyed over radio links. Recent new developments such as DECT New Generation now also offer wideband 7 kHz voice transmission, a super-wideband   
14 kHz service, different data services and video surveillance. While these technological advances are well received, because they are reflecting the general trend towards multimedia devices, they are also requiring a lot more bandwidth.

DECT based softphones are one of the technologies in use as a telephony solution in the business market, which is increasing in all regions worldwide with annual growth figures >10%. By the year 2017, the Global Industry Analysts (GIA) group project market adoption of 2.9 million units (GIA online, 2011). This steady migration from traditional desk based telephones does result in users adopting new device solutions for their audio connectivity. The headset is now a prime audio device chosen by softphones users as PCs are not shipped with the traditional handset that a desk based hard phone would be supplied with. Whether it be in a contact centre environment or office environment, the use of PC based telephony which delivers wideband audio is leading to behaviour change within these organisations. Users equipped with headsets that deliver enhanced (wideband) audio may use the same devices to stream music from their connected PCs. Therefore, such users who may not be on an active telephony call may still be in a wideband audio media link between telephony calls.

DECT technology is used in wireless headsets solutions. Many large Enterprises recognise the benefits that these wireless devices bring and promote deployment of them within their businesses for their office users as well as for their more traditionally contact centre users. Such large enterprises may occupy single buildings with staff levels in excess of 500 users, each one requiring a wireless device. Within city business areas, adjacent large organisations may also seek to use the same wireless technology.

As DECT is a very reliable and cost effective system, new applications are being developed using this technology. One new feature of DECT is the ‘Ultra Low Energy’ (ULE) operation mode which has been developed during 2012. This allows battery operated devices to work for up to 10 years without changing the battery. The ULE mode, together with the other DECT properties, makes this technology a candidate for use in machine-to-machine applications, such as home automation applications which will increase the number of DECT terminals massively. This ULE mode can also operate in the current DECT spectrum. The combined effect of successful softphone adoption, wideband telephony, music at work and deployment of wireless devices is causing already today density issues within the existing spectrum available leading to deployments being affected or restricted. In addition new services are starting to be deployed such as video applications and data applications like home control. An investigation will be necessary to provide more specific data on the spectrum requirements.

### What are the specific advantages of the band 1900-1920 MHz

Most technical documents are already available. The carrier numbers and positions for the use of DECT in the 1900-1920 MHz band are already defined (see annex F of ETSI EN 300 175-2 [16]) as consequence of the IMT allocation. The Harmonised standard for DECT over this band is already available as part of the IMT-2000 set. It is the ETSI EN 301 908-10 [15] (latest release, v4.1.1).

Immediate product implementation is possible from the technical point of view. It should be noted that the frequencies 1900-1930 MHz are already in use by DECT in non EU countries and that there are already products (> 100 million of devices) in operation over these frequencies. Near all DECT chipset and RF parts vendors are already providing components compatible with the proposed new allocation. There is no other band where the DECT extension is as simple and immediate. This, combined with the proposed license-exempt regime, will make possible the real usage of the band by the public in the very short term.

A designation within the adjacent band 1900-1920 MHz to DECT will provide a single continuous block of up to 40 MHz. This, in combination with the use of already defined HLM (High Level Modulation - up to 64 QAM) would make possible the introduction of additional broadband services via DECT. This would make also possible the further evolution of the standard towards OFDMA. A maximum bitrate of 1Gbit/sec is theoretically achievable over the combined 40 MHz block using already proposed evolutions of the standard.

If a contiguous designation is given for the DECT technology, two additional RF carriers can be obtained by avoiding guard spaces.

### Possible way forward for implementation of DECT in 1900-1920 MHz

It is understood that the DECT proposal is made on an application-neutral basis and can also be considered for a technology-neutral approach using general authorisation (exemption from individual licence).

It should be noted that the request in ETSI TR 103 149 [34] does not include the requirement for DECT to access spectrum exclusively, e.g. as a pre-requisite to ensure high quality of service. Therefore, the status of DECT in a possible extension band would be different compared to the current exclusivity of accessing spectrum in the range 1880-1900 MHz.

DECT use cases are primarily indoor but not exclusively. Therefore, an indoor restriction in the band 1900-1920 MHz may be an option for consideration, although not the preferred one. Outdoor usage is possible under the current regulations in the band 1880-1900 MHz.

## Public Protection and Disaster Relief

Within CEPT, the Unpaired 2 GHz bands (1900-1920 MHz and 2010-2025 MHz) are under discussion as a candidate for a harmonised solution above 1 GHz for ad-hoc PPDR network uses including, for some countries, PPDR broadband air-to-ground applications. Broadband PPDR temporary additional capacity (also known as “hot-spot” or “local area” networks) are supposed to provide additional local coverage at the scene of the incident in order to provide the necessary communication facilities to PPDR users in addition to those provided through the Wide Area network (WAN) or where the WAN radiocommunications are limited or not available. This additional capacity may be provided by Ad-hoc networks or other means (such as additional temporary base stations of the WAN) and are supposed to have high capacity and support PPDR users with low mobility. Ad-hoc networks may operate in the same (i.e. in a form of an ad-hoc micro-cell deployed at the event’s scene) as well as in a different frequency band.

PPDR organisations may also have requirements for broadband air-to-ground applications e.g. from UAVs or helicopters to support PPDR operations. These typically involve a video stream being relayed from a camera mounted on an airborne platform to a monitoring station on the ground. The requirements for broadband air-to-ground PPDR spectrum within CEPT have not been evaluated in detail in ECC Report 199 [23]. However some countries have provided a national estimate of their broadband air-to-ground spectrum needs. Based on this information, a realistic estimate for airborne PPDR is under investigation. For broadband air-to-ground usage, also cross-border coordination needs to be studied.

Possible synergies between these applications and PMSE use described in section 3.2 (Programme Making and Special Events) are further explored, since the same technologies / equipment may be used and the same technical framework might aply.

## Synergies between the proposed short list of selected use

* **Applications under general authorisation (DECT / SRD)**

DECT, SRD (both candidates are seeking an allocation under a general authorisation regime). There may be a possibility of having a common set of technical parameters to enable equal spectrum access.

One possibility: General authorisation enabling DECT extension as well as application and technology-neutral access to spectrum in line with principles set out in CEPT Reports 14 and 44 (SRD strategy and principles).

During the Call for Inputs, the responding administrations clearly indicated that DECT should operate under a generic SRD regulation on a shared basis with other technology on a non-protected non-interfered basis. Spectrum access techniques should be mutually compatible and frequency segmentation amongst such applications should be avoided. It is important that the regulation also in practice provides an opportunity for alternative technologies to use the spectrum so that a competitive market is created.

Once defined with appropriate mitigation techniques and restrictions, DA2GC could share with a DECT/SRD regulation to be introduced on a non-protection, non-interference basis without affecting the DA2GCS, as an optimised scenario.

* **Video Links and cordless cameras (PMSE / PPDR)**

Ad-hoc PPDR and PMSE, using the same technical framework and equipment, i.e. temporary video links or cordless cameras. There may be a possibility of having a common set of technical parameters for spectrum access. It should be noted that the assumption is that coordination and the associated usage demand will be dealt with on a national level. It should be noted that video applications such as surveillance cameras under general authorisations are not included in this usage block.

One possibility: Extended tuning range for video links and cordless cameras, including both PMSE and PPDR usage. The 2010-2025 MHz band is directly adjacent to the 2025-2110 MHz band that is already part of the tuning range for video PMSE applications.

For ad-hoc PPDR, other frequency options are also under discussions in CEPT.

The unpaired 2GHz bands may ultimately offer only a small amount of available spectrum for ad-hoc PPDR and practical difficulties of sharing with PMSE are envisaged in unplanned event situations. Technology issues may also arise due to the different trends towards using DVB-based technology in the PMSE community for video links and LTE-based technologies for BB-PPDR solutions. The amount of support expressed for ad-hoc PPDR solutions in the Call for Inputs has been very limited. Nevertheless, the bundling of video links and cordless cameras under a co-ordinated approach leaves the door open for dedicated ad-hoc PPDR broadband applications in the 2 GHz unpaired bands under the same technical environment.

During the Call for Inputs, all PMSE proponents indicated that they do not consider PMSE to share with unlicensed applications such as DECT/SRD. Usage of these license free devices in the same band where essential professional services (PMSE/PPDR) are being deployed impairs the error free use of these professional services. This notion has also been provided by the one response from a PPDR solutions provider. Therefore, it is not foreseen to have co-frequent use of the two usage blocks PMSE/PPDR and DECT/SRD.

Within the PMSE/PPDR block, coordination between PMSE and PPDR is essential for an optimised scenario between those two uses of the proposed shortlist, in order to profit from the synergies between them. The UK’s experience on such a coordination process, currently in place, is presented below:

For a number of major events the supply of spectrum allocated for PMSE is not sufficient to meet the demands of the event itself, e.g. British Grand Prix, Open golf Championship, National events etc. In these circumstances. it is necessary to source additional spectrum from alternative bands and users. In the UK it is common to source and coordinate additional spectrum for PMSE from the PPDR services.

An example of this is wireless camera use in the band 2302-2380 MHz that is currently allocated to PPDR. For peak demand events where PMSE spectrum demand cannot be met from that allocated to PMSE access to 2302-2380 MHz is often arranged in order to supplement the PMSE core bands.

In addition, there are some circumstances where PPDR may require supplementary spectrum and there are arrangements in place whereby PPDR services can coordinate access to spectrum allocated to PMSE.

The UK’s experience shows that the need for supplementary spectrum for PMSE or PPDR does not generally occur for the same event i.e. when there is excessive demand for PMSE spectrum at an event PPDR interest is low and vice versa. If this is not the case a significant effort is put in to coordinating and accommodating the conflicting requirements. Should an emergency occur at an event where PMSE is utilising PPDR spectrum it is our view that the event itself would unlikely continue and spectrum would revert back to PPDR.

It is highlighted that PMSE can only access PPDR spectrum where use for PPDR is intermittent in both location and time thereby affording PMSE the opportunity to interleave with PPDR use. Similarly, PPDR access to PMSE spectrum is for applications that are specific to a particular time and location so can be coordinated with PMSE requirements. In the event that the unpaired 2 GHz spectrum was made available for ‘always on, everywhere’ use by PPDR there would be no opportunity for PMSE to share access.

* **Conclusions**

As a result of the synergies between PMSE and PPDR, as well as between DECT and SRD, the shortlist indicated in the EC Mandate, composed of five potential harmonised uses of the 1900-1920 MHz and 2010-2025 MHz frequency bands (DA2GC, PMSE, PPDR, DECT and SRD), is considered to be adequately studied by using three usage blocks as presented in the following Figure 8.

Figure 8: Synergies between the proposed short list of selected use

As a result, the compatibility / sharing scenarios that are being studied within the aim of the outline of the response to the Commission consider as a basis the three usage blocks set out in Figure 8.

1. EC Mandate

|  |  |
| --- | --- |
|  | EUROPEAN COMMISSION  Communications Networks Content & Technology Directorate-General  Electronic Communications Networks & Services  **Spectrum** |

Brussels, 10 October 2012

DG CONNECT/B4

**RSCOM12-17 rev3**

**ADOPTED**

**RADIO SPECTRUM COMMITTEE**

**Working Document**

**Opinion of the RSC  
pursuant to Advisory Procedure under Article 4 of Regulation 182/2011/EU and Article 4.2 of Radio Spectrum Decision 676/2002/EC**

**Subject: Mandate to CEPT to undertake studies on the harmonised technical conditions for the 1900-1920 MHz and 2010-2025 MHz frequency bands in the EU**

*This is a Committee working document which does not necessarily reflect the official position of the Commission. No inferences should be drawn from this document as to the precise form or content of future measures to be submitted by the Commission. The Commission accepts no responsibility or liability whatsoever with regard to any information or data referred to in this document.*

**Mandate to CEPT   
to undertake studies on the harmonised technical conditions for the 1900-1920 MHz and 2010-2025 MHz frequency bands ("unpaired terrestrial 2 GHz band") in the EU**

**PURPOSE**

The purpose of the UMTS Decision of 1999[[7]](#footnote-7), which covered the frequency bands 1900-1980 MHz, 2010-2025 MHz and 2110-2170 MHz ('terrestrial 2 GHz band'), was to initiate the introduction of UMTS in the EU in a coherent manner. The UMTS Decision expired on 22 January 2003 and fulfilled its objectives. Any outstanding or related issues after 2003 such as on spectrum allocation, licensing or re-farming have been governed by the EU regulatory framework in electronic communications as well as the Radio Spectrum Decision 676/2002/EC since 2002.

Even if licences for the unpaired terrestrial 2 GHz band, comprising the TDD bands 1900-1920 MHz and 2010-2025 MHz, have been granted to mobile operators in the EU for many years, the proven lack of use of these bands (see document RSCOM12-05) necessitates new harmonisation measures in order to ensure effective and efficient spectrum use in line with the EU regulatory framework and the "use it or lose it" approach endorsed by the Commission to the extent possible under the existing regulatory framework.

Technical conditions for the provision of electronic communications services (ECS) in the unpaired terrestrial 2 GHz band have been developed under the initial Commission's Mandate to CEPT[[8]](#footnote-8) in CEPT Report 39[[9]](#footnote-9). Unless demonstrated in the course of the work to be done under this Mandate that new technological developments in electronic communications should be taken into account, there is no need to revise those results. Therefore, this Mandate should cover as a priority uses not covered by CEPT Report 39, primarily non-ECS uses.

Therefore, the purpose of this Mandate is to assess and identify alternative uses of the unpaired terrestrial 2 GHz band other than for the provision of mobile electronic communications services (as introduced by the UMTS Decision) as well as develop relevant least restrictive technical conditions for spectrum use. The deliverables should aim at ensuring effective and efficient spectrum use by one or more applications while also exploiting the possibility of beneficial sharing arrangements between different applications.

**JUSTIFICATION**

Pursuant to Article 4(2) of the Radio Spectrum Decision[[10]](#footnote-10) the Commission may issue mandates to the CEPT for the development of technical implementing measures with a view to ensuring harmonised conditions for the availability and efficient use of radio spectrum necessary for the functioning of the internal market. Such mandates shall set the tasks to be performed and their timetable.

In response to the Mandate by the Commission**Error! Bookmark not defined.**, CEPT Report 39 lays down least restrictive harmonised technical conditions for use of the terrestrial 2 GHz band for the provision of two-way mobile electronic communications services. However, the technical conditions for the unpaired (TDD) bands impose significant restrictions regarding the amount of usable spectrum or the admissible transmit power levels in order to protect operations in adjacent frequency bands, mainly the FDD uplink band above 1920 MHz, from harmful interference.

Currently, the frequency band 1900-1920 MHz is licensed to mobile operators for the provision of electronic communications services in most EU Member States, whereby the licences are mainly limited to UMTS/IMT-2000 TDD technology[[11]](#footnote-11). On the other hand, the frequency band 2010-2025 MHz is licensed to mobile operators in just few Member States for the provision of electronic communications services, in some cases in a technology-neutral way. Both bands are not used in the EU. Recently, the lack of interest of mobile operators for spectrum in the unpaired terrestrial 2 GHz band has been demonstrated during the auctions in Italy and Portugal in 2011, where the 2010-2025 MHz band was put on offer but remained unsold.

Therefore, the effective and efficient use of the 1900-1920 MHz and 2010-2025 MHz frequency bands is handicapped by the lack of business interest of current rights' holders or other potential stakeholders from the mobile domain. This may be explained with the limited overall bandwidth of each of these bands and the coexistence limitations between multiple mobile networks[[12]](#footnote-12), which reduce the number of independent mobile broadband operators in each band (operating on a channel of at least 10 MHz) to one or two. The lack of demand for unpaired 2 GHz spectrum has lead to the absence of equipment and an ecosystem. Therefore, the Commission considers that there is no viable harmonisation option within the mobile broadband context for both bands so that it becomes necessary to focus on alternative scenarios for the harmonised use of the unpaired terrestrial 2 GHz band that can justify demand and demonstrate socio-economic benefits.

In this regard, the principles and objectives set out by the Radio Spectrum Policy Programme (RSPP) must be duly taken into account, as well as the spectrum needs of specific Union policies[[13]](#footnote-13) such as improving energy saving and efficiency, public protection and disaster relief (PPDR), the Internet of Things (IoT), programme making and special events (PMSE)[[14]](#footnote-14) as well as for innovative applications that may have a major socio-economic impact and/or potential for investment.

Furthermore, as a result of the public consultation of the Commission on the introduction of EU-wide technical harmonisation conditions for the terrestrial 2 GHz band (15 November 2011 - 28 January 2012)[[15]](#footnote-15), a number of respondents proposed alternative uses of the 1900-1920 MHz and 2010-2025 MHz frequency bands. These include broadband PPDR, DECT, Direct-Air-to-Ground Communications (DA2GC), PMSE (e.g. wireless cameras), short range devices (SRD), backhaul relay links of mobile networks, mobile IP services with quality-of-service management based on the IEEE 802.20 standard. Some of these proposals correspond to sectors or policies outside of wireless broadband, which have been identified by the RSPP as requiring special attention, and all are aligned with the RSPP's policies and objectives.

In view of the above, the Commission services have identified the following *shortlist* of potential harmonised uses of the 1900-1920 MHz and 2010-2025 MHz frequency bands to be given priority[[16]](#footnote-16) in this Mandate:

1. PPDR, most likely with preference to ad-hoc (non-permanent) PPDR networks.
2. PMSE, preferably for use by wireless cameras**Error! Bookmark not defined.**.
3. Short-range devices (SRD), preferably for improving energy saving and/or energy efficiency.
4. DECT[[17]](#footnote-17), preferably in the 1900-1920 MHz band.
5. Broadband Direct Air-to-Ground Communications (BDA2GC), preferably in a paired spectrum arrangement.

The Commission notes that also other frequency bands are currently under investigation in CEPT for some of the radio applications above.

It can be assumed that some of the applications above being temporary or local in nature would not utilise exclusively the total available spectrum in the unpaired terrestrial 2 GHz band. Therefore, *shared use* between the different applications should be studied in order to ensure efficient spectrum use. In this regard, appropriate least restrictive technical conditions should be developed both for the identified specific application and for any possible sharing arrangement.

The Commission notes that the CEPT/ECC has already launched studies on the alternative use of the 1900-1920 MHz and 2010-2025 MHz frequency bands[[18]](#footnote-18), which may contribute to timely deliverables in response to this Mandate.

Given the proven long-term lack of use of the unpaired 2 GHz spectrum under the current assignments and the foregoing RSC work before the adoption of the RSPP, this Mandate may be issued in advance of the outcome of the inventory process set up by the RSPP. The deliverables of this Mandate should be reflected in the EU spectrum inventory process.

**TASK ORDER AND SCHEDULE**

CEPT is herewith mandated to undertake work to identify use(s) of the *unpaired terrestrial 2 GHz band* other than for the provision of mobile electronic communications services through terrestrial cellular networks pursuant to the UMTS Decision and the most appropriate technical criteria for spectrum use as well as, if appropriate, sharing arrangements between multiple applications, in order to meet EU spectrum policy objectives and foster economies of scale in the internal market.

In the work carried out under the Mandate, the overall policy objectives of the RSPP, such as effective and efficient spectrum use and the support for specific Union policies shall be given utmost consideration. In implementing this mandate, the CEPT shall, where relevant, take utmost account of EU law applicable and support the principles of service and technological neutrality, non-discrimination and proportionality insofar as technically possible. CEPT is also requested to collaborate actively with the European Telecommunications Standardisation Institute (ETSI) which develops harmonised standards for conformity under Directive 1999/5/EC.

CEPT is hereby mandated to undertake the following tasks:

1. Assess and identify uses other than mobile electronic communications services delivered through terrestrial cellular networks and define the common minimal (least restrictive) technical conditions. These conditions should be sufficient to avoid interference with services or radio applications in adjacent bands, ensure co-existence with other services or radio applications in the same band, and facilitate cross-border coordination, also at the EU outer borders.
2. In performing task (1), consider the following non-ECS uses in line with the priorities of the RSPP: broadband PPDR, PMSE, short-range devices and DECT[[19]](#footnote-19). This is without prejudice to the consideration of alternative uses for electronic communications services in line with EU spectrum policy objectives, such as Broadband Direct-Air-To-Ground Communications.
3. In performing task (1) as specified by task (2) and given the limited temporal or geographical scope of one or more of the radio application under consideration, assess and justify the possibility of spectrum sharing amongst the radio applications under consideration and, if necessary, develop common technical sharing conditions which may include *inter alia* spectrum access rules, channelling arrangements or power emission limits that are sufficiently precise for the development of EU-wide equipment.

CEPT should provide deliverables according to the following schedule:

Table 4: Deliverable’s schedule as specified in the EC Mandate

| **Delivery date** | **Deliverable** | **Subject** |
| --- | --- | --- |
| June 2013 | Interim Report from CEPT to the Commission | Description of work undertaken and interim results under this Mandate. |
| November 2013[[20]](#footnote-20) | Final Draft Report from CEPT to the Commission on selected use(s). | Description of work undertaken and final results under tasks (1) and (2) of this Mandate. |
| March 2014 | Final Report from CEPT to the Commission on selected use(s), taking into account the outcome of the public consultation | Description of work undertaken and final results under tasks (1) and (2) of this Mandate taking into account the results of the public consultation |
| June 2014**Error! Bookmark not defined.** | Final Draft Report from CEPT to the Commission. | Description of work undertaken and final results under this Mandate. |
| November 2014 | Final Report from CEPT to the Commission. taking into account the outcome of the public consultations | Description of work undertaken and final results under this Mandate taking into account the results of the public consultations |

In addition, CEPT is requested to report on the progress of its work pursuant to this Mandate to all meetings of the Radio Spectrum Committee taking place during the course of the Mandate.

The Commission, with the assistance of the Radio Spectrum Committee and pursuant to the Radio Spectrum Decision, may consider applying the results of this mandate in the EU, pursuant to Article 4 of the Radio Spectrum Decision.

1. RESULTS OF THE CALL FOR INPUTS

The present Annex provides the results of the Call for Inputs on the outline of the response to the Commission in respect of the development of a CEPT response to the EC Mandate “To undertake studies on the harmonised technical conditions for the 1900-1920 MHz and 2010-2025 MHz frequency bands (‘Unpaired terrestrial 2 GHz bands’) in the EU”.

**Background**

The present outline of the response to the Commission describes the shortlist of potential harmonised uses of the 1900-1920  MHz and 2010-2025 MHz frequency bands in accordance with the EC Mandate to CEPT “To undertake studies on the harmonised technical conditions for the 1900-1920 MHz and 2010-2025 MHz frequency bands (“Unpaired terrestrial 2 GHz bands”) in the EU”.

The full range of source information has not been available to the extent that an ECC consultation in the formal sense could have been started at the ECC meeting in 5-8 November 2013. Therefore, the ECC decided instead to make a ‘Call for Inputs’ in order to gather relevant information from stakeholders in a timescale aligned with the requirements of the ‘Unpaired terrestrial 2 GHz bands’ Mandate. The consultation ended on 20th December 2013.

The following questions were put forward for consideration in addition to the outline of the response to the Commission on the shortlist of potential harmonised uses:

1. General questions
   1. **What is your view on the preferred scenarios / uses for the bands 1900-1920 MHz and 2010-2025 MHz as set out in the outline of the response to the Commission? Please, justify your answer by indicating the associated economic and other benefits of your preference.**
   2. In the outline of the response to the Commission it is suggested placing the shortlist of potential harmonised uses of the 1900-1920 MHz and 2010-2025 MHz frequency bands, proposed for further study in the EC Mandate (as detailed in Annex 4), into 3 defined categories (see section 3.6 of the outline of the response to the Commission on Synergies between the proposed short list of selected use). **Do you agree with this approach? (Yes/No) If not please explain in detail why.**
2. DECT and SRD

Two of the potential uses of the 1900-1920 MHz and 2010-2025 MHz frequency bands proposed for study in the EC Mandate are DECT (1900-1920 MHz) and SRDs. Both uses would normally employ adequate mechanisms to access the spectrum equitably and operate under a general authorisation framework. The approach is application-neutral and technology-neutral as much as possible and in line with the principles set out in CEPT Report 14 and CEPT Report 44.

**Do you agree that SRD and DECT may be deployed and share the spectrum under a common technical and regulatory framework to foster a more efficient use of spectrum and future innovation? (Yes/No) If not, please indicate why.**

1. PMSE and ad-hoc PPDR

Two of the potential uses of the 1900-1920 MHz and 2010-2025 MHz frequency bands proposed for study in the EC Mandate are PMSE and ad-hoc PPDR. Both proposed uses of the band are to provide temporary links both fixed and mobile (incl. airborne such as video links from/to helicopters or unmanned air vehicles), where these frequency bands would be included in an extended harmonised tuning range for video cameras and video links. The proposal in the outline of the response to the Commission is that the same technical framework and same equipment can be used to meet the operational needs of both PMSE and PPDR users.

**Do you agree that PMSE and ad-hoc PPDR show sufficient similarities to share the same technical framework to foster a more efficient use of spectrum and future innovation? (Yes/No). If not, please indicate why.-**

Comments have been received from:

1. Deutsche Telekom
2. TriaGnoSys (affiliated to aircraft cabin manufacturer Zodiac Aerospace)
3. Riedel (provider of PMSE solutions)
4. NPO (Nederlandse Publieke Omroep; Netherlands Public Broadcasting)
5. Vislink (provider of PMSE solutions)
6. IRT (Institut für Rundfunktechnik) (research institute of the public broadcasters of Germany, Austria, and Switzerland)
7. France
8. DECT Forum
9. Sweden
10. Lufthansa Systems
11. Netherlands
12. Selex ES (inter-alia provider of PPDR solutions)
13. British Airways
14. Telefónica S.A.
15. Multi-operators’ response from Bouygues Telecom, Orange, and SFR (Société Française de Radiotéléphone)
16. Germany
17. BT (British Telecommunications PLC)

All the comments are included in Annex 2 of Document FM(14)021 [xxx.

**Summary of the responses**

The table below includes an indicative overview of the support for applications (whereby some comments rather support the concept than specific applications, and some respondents may support different applications in different ranges).

|  |  |
| --- | --- |
| **Application** | **Supported by number of responses** |
| Broadband DA2GC | 1, 2, 7, 10, 11, 13, 14, 16, 17 |
| DECT | 8, 11, 16 |
| SRDs | 9, 11, 16 |
| PMSE | 3, 4, 5, 6, 7, 11, 16 |
| ad-hoc PPDR | 12, 16 |
| Other usage | 11, 15 |

1. General questions
   1. **What is your view on the preferred scenarios / uses for the bands 1900-1920 MHz and 2010-2025 MHz as set out in the outline of the response to the Commission? Please, justify your answer by indicating the associated economic and other benefits of your preference.**

**DA2GCS:**

*Deutsche Telecom and TriaGnoSys expressed the support of a harmonised FDD solution in 1900-1910 MHz paired with 2010-2020 MHz. Telefonica also expressed their preference for an FDD solution for DA2GCS in the 2 GHz Unpaired Bands. Lufthansa Systems expressed the view that a TDD solution for DA2GCS in the 2 GHz Unpaired Bands should not be excluded from considerations, preferably for the 1900-1920 MHz band. BT also expressed their preference that the band 1900 – 1920 MHz is made available for DA2GC applications. No responder declared a preference for a DA2GCS TDD solution in the 2010-2025 MHz band.*

*France indicated that DA2GC could operate in the 2 GHz Unpaired Bands on a shared basis and the views expressed by other DA2GCS proponents go in the same direction, provided that coexistence conditions are clearly identified. Germany stated to support the preferred scenarios / uses as set out in the outline of the Call for Inputs. Netherlands stated that the unpaired band could partly be used for DA2CG. British airways expressed their support for a harmonised solution for DA2GCS without indicating a preferred technical solution. One of the two options defended by Lufthansa Systems points out the entire 20 MHz in the lower band to DA2GC for TDD usage leaving the 2010-2025 MHz for use by one or several of other applications.*

*Sweden finds it difficult to judge about economic benefits or other benefits that could be associated from an introduction of BDA2GC for a number of reasons expressed in the response. Generally a higher frequency band such as investigated by the FCC at the 14 GHz range would be preferred due to a lower opportunity cost. The Netherlands also indicated that economic benefits are not really clear yet but at least a reservation for this application may be advisable at higher frequencies.*

**PMSE:**

*Riedel, NPO, IRT, and Vislink expressed support for PMSE applications in the 2 GHz Unpaired Bands. The major benefits are seen in the slight expansion of the tuning range and preferable propagation conditions enabling non-line-of-sight video links compared to higher frequency ranges.*

*The four responding administrations also indicated to see the possibility for PMSE in the 2 GHz Unpaired Bands. Other responders such as DA2GCS proponents indicated to see sharing possibilities with PMSE applications.*

**DECT:**

*The DECT Forum expressed their view to make also available the 1900-1920 MHz band for DECT and refers to growth possibilities for higher rate data services, video surveillance and general home automation services, and especially M2M applications (for the latter one, an excerpt of the ETSI SRdoc has been provided).*

*Sweden does not predict a long-term growth of the DECT market, and estimates the benefits associated to a harmonisation of additional frequency spectrum are therefore limited.*

**SRD:**

*Sweden believes that with the right regulatory and technical conditions, an introduction of SRD in these bands potentially has a very high contribution to economic benefits in Europe.*

*France is of the view that based on appropriate mitigation techniques and restrictions, DA2GC could share with video applications, and an SRD regulation could also be introduced on a non-protection, non-interference basis without affecting the other services, as an optimised scenario.*

*The Netherlands proposed to consider metering (smart metering, smart grids and smart cities) in the unpaired bands, taking note that the needed frequency ranges are dependent on a country’s geography and the average construction of houses and buildings. It is also referred that a number of bands proposed for metering, such as the 870-876 MHz, are not available in a substantial number of countries.*

**Other use, outside the indicated preferred scenarios/uses:**

*Two responses indicated other use, outside the indicated preferred scenario/uses:*

*Bouygues Telecom, Orange, and SFR stated that the current allocation of the unpaired terrestrial 2 GHz bands to the mobile network operators sould remain as one of the possible alternatives. The main point of this contribution is to indicate the recent availability of mass-market handsets on the 2.1 GHz TDD bands. Such handsets are the same as those which also include the 2.3 GHz TDD band and the 2.6 GHz TDD band, in addition to all European FDD LTE bands. No statement was made with regard to the availability of network solutions in the unpaired bands (the main issue stated in the past has been the DL-emission limitations to be spectrum compatible with other applications in the adjacent spectrum).*

*This usage concept brought forward by the three operators may include TDD-FDD aggregation on hotspots and for M2M applications. The three operators are of the view that each potential harmonised use in the shortlist should be assessed against the use of the unpaired 2GHz bands for TDD-FDD aggregation on hotspots and for M2M. Telefonica mentioned the various licenses they hold in the 1920-1980 MHz/ 2110-2170 MHz across Europe and, in this context indicated that any solution in the 2 GHz Unpaired bands has to be spectrum compatible, i.e. protection of the adjacent services needs to be fulfilled.*

*The Netherlands introduced the view that radio amateur (satellite) use as well as wireless smart metering, smart grids and smart city networks should also be considered.*

* 1. In the outline of the response to the Commission it is suggested placing the shortlist of potential harmonised uses of the 1900-1920 MHz and 2010-2025 MHz frequency bands, proposed for further study in the EC Mandate (as detailed in Annex 1), into 3 defined categories (see section 3.6 of the outline of the response to the Commission on synergies between the proposed shortlist of selected use. **Do you agree with this approach? (Yes/No) If not please explain in detail why.**

*From almost all responses, a high level of support has been expressed for the approach adopted by CEPT. Some responses indicate explicit possibilities or concerns that may need further investigations or refer to insufficient information:*

* *Deutsche Telekom, TriaGnoSys see sharing of the DA2G forward link (ground-to-air) with PMSE cordless camera links is feasible under specific conditions. Such sharing feasibility is also expected to be valid for applications like SRD and DECT, in particular if low power, low duty cycle, DCS (Dynamic Channel Selection) and/or a restriction to in-house-only operation would apply for these applications.*
* *The need to be more precise on synergies, especially between PPDR and PMSE as well as on possibilities to coordinate ad hoc PPDR and PMSE usage.*
* *Telefonica supports the approach but needs also proper consideration of existing licenses and socio-economic studies detailing the synergies.*
* *DECT: precise usage should be further clarified, especially with regards to the handling of DECT video/video surveillance applications under the concept with the DECT/SRD and PMSE/ad-hoc PPDR blocks.*
* *The DECT Forum expressed itself to be unable to support the common DECT/SRD approach due to lack of information on potential SRD usage.*

1. DECT and SRD

Two of the potential uses of the 1900-1920 MHz and 2010-2025 MHz frequency bands proposed for study in the EC Mandate are DECT (1900-1920 MHz) and SRDs. Both uses would normally employ adequate mechanisms to access the spectrum equitably and operate under a general authorisation framework. The approach is application-neutral and technology-neutral as much as possible and in line with the principles set out in CEPT Report 14 and CEPT Report 44.

**Do you agree that SRD and DECT may be deployed and share the spectrum under a common technical and regulatory framework to foster a more efficient use of spectrum and future innovation? (Yes/No) If not, please indicate why.**

* *Several PMSE proponents indicate that they do not consider PMSE should share with unlicensed applications such as DECT/SRD. Usage of these licence-free devices in the same band where essential professional services (PMSE/PPDR) are being deployed impairs the error free use of these professional services. This notion has also been provided by the one response from a PPDR solutions provider.*
* *The responding administrations clearly indicated that DECT should operate under a generic SRD regulation on a shared basis with other technology on a non-protected non-interfered basis. Spectrum access techniques should be mutually compatible and frequency segmentation amongst such applications should be avoided. It is important that the regulation also in practice provide an opportunity for alternative technologies to use the spectrum so that a competitive market is created. SRD application spectrum access options (for sharing considerations) mentioned in the responses include low duty cycle and also LBT+AFA, DAA options.*

1. PMSE and ad-hoc PPDR

Two of the potential uses of the 1900-1920 MHz and 2010-2025 MHz frequency bands proposed for study in the EC Mandate are PMSE and ad-hoc PPDR. Both proposed uses of the band are to provide temporary links both fixed and mobile (incl. airborne such as video links from/to helicopters or unmanned air vehicles), where these frequency bands would be included in an extended harmonised tuning range for video cameras and video links. The proposal in the outline of the response to the Commission is that the same technical framework and same equipment can be used to meet the operational needs of both PMSE and PPDR users.

**Do you agree that PMSE and ad-hoc PPDR show sufficient similarities to share the same technical framework to foster a more efficient use of spectrum and future innovation? (Yes/No). If not, please indicate why.**

*Two major concerns have been expressed concerning the PMSE/ ad-hoc PPDR sharing the same technical framework which seems to require additional discussions:*

* *Several PMSE proponents indicated to support the categories/concept to use the same technical framework but also consider that PMSE/PPDR actual sharing might be difficult to achieve and coordination in certain situations (e.g. disaster spot) not being practicable. Others were more optimistic concerning this aspect and indicated that coordination and licensing conditions should be done on a national level.*
* *The need for more information, to support the on-going compatibility studies and also to clarify the precise PMSE/PPDR synergies was indicated. This may include DVB-T vs LTE considerations, 1-way/2-way communication needs and that PPDR does not only include video applications.*

**Other uses suggested in the aim of the Call for Inputs**

About **other uses** brought up in the Call for Inputs, the following is noted:

* *MOBILE*:

In one contribution from three mobile operators, the desire to maintain the current allocation of the unpaired terrestrial 2 GHz bands to the mobile network operators is expressed as one of the possible alternatives. This usage concept brought forward by the three operators is meant to include TDD-FDD aggregation on hotspots and M2M applications. In addition, the three operators are of the view that each potential harmonised use in the shortlist should be assessed against the use of the unpaired 2GHz bands for TDD-FDD aggregation on hotspots and for M2M.

On the other hand, it has to be noted that the purpose of the Mandate on the “Unpaired terrestrial 2 GHz bands” is to assess and identify alternative uses of the unpaired terrestrial 2 GHz band other than for the provision of mobile electronic communications services. Consequently, apart from the arguments presented, this option was considered to be out of the scope of this Mandate.

* *AMATEUR (SATELLITE)*:

A proposal to consider the amateur (satellite) service use in the unpaired bands for cognitive radio experiments under controlled conditions was presented, under the argument that frequency use for the radio amateur service is currently under pressure.

It can be seen from the RR Article 5 and the ECA Table that the amateur-satellite service always follows an amateur service allocation. As no amateur service allocation exists at the moment for the 2 GHz Unpaired Bands, it may be a long process to introduce such an allocation. Therefore, any activity within CEPT on this matter is considered to need sufficient support and a clear description of the demand, so as to conduct all necessary studies. It is as well to note that amateur-satellite service allocations already exist for the bands 1260-1270 MHz and 2400-2450 MHz, therefore it is suggested not to consider the proposed amateur-satellite usage in the 2 GHz Unpaired Bands.

1. Current authorisations in the bands 1900-1920 MHz / 2010-2025 MHz

ECO Report 003 [9] on the licensing of mobile bands in CEPT includes in the version from 2 July 2013 the following information (information update indicated in brackets):

1. **Austria (March 2013)**

**1900-1920 MHz and 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequency band licensed** | **Technology in use (optional)** | **Licence duration, tradability** |
| Hutchison 3G Austria GmbH | 1915.1 – 1920.1 MHz |  | Until Dec. 2020  tradeable |
| A1 Telekom Austria AG | 1900.1 – 1910.1 MHz |  | Until Dec. 2020  tradeable |
| T-Mobile Austria GmbH | 1910.1 – 1915.1 MHz  2019.9 – 2024.7 MHz |  | Until Dec. 2020  tradeable |

1. **Belgium (January 2012)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration. tradability** |
| Belgacom Mobile (Proximus) | 1914.9-1920.3 MHz |  | 15/03/2001-15/03/2021  Tradable |
| Mobistar | 1909.9-1914.9 MHz |  | 15/03/2001-15/03/2021  Tradable |
| KPN Group Belgium (Base) | 1899.9-1904.9 MHz |  | 15/03/2001-15/03/2021  Tradable |

1. **Belarus (not included yet in published ECO Report 03)**

**1900-1920 MHz and 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequency band licensed** | **Technology in use (optional)** | **Licence duration, tradability** |
| vacant | 1900-1920 MHz | UTRA TDD | Awaiting of a decision of State Commission for Radio Frequencies |
| vacant | 2010-2025 MHz | UTRA TDD | Awaiting of a decision of State Commission for Radio Frequencies |

1. **Bosnia and Herzegovina (March 2013)**

**1900-1920 MHz/2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use**  **(optional)** | **Licence duration, tradability** |
| Telekomunikacije RS | 1910 – 1915 MHz | UTRA TDD | 01.04.2009. -31.03.2024,  non-tradable |
| BH Telecom | 1900 – 1905 MHz | UTRA TDD | 01.04.2009. -31.03.2024,  non-tradable |
| HT Mostar | 1905 – 1910 MHz | UTRA TDD | 01.04.2009. -31.03.2024,  non-tradable |

1. **Bulgaria (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Mobiltel ЕAD | 2010-2015 MHz | UTRA TDD | 25.04.2005 - 25.04.2025, transferable |
| Cosmo Bulgaria Mobile EAD | 2020-2025 MHz | UTRA TDD | 25.04.2005 - 25.04.2025, transferable |
| Bulgarian Telecommunications Company AD | 2015-2020 MHz | UTRA TDD | 25.04.2005 - 25.04.2025, transferable |

1. **Croatia (January 2012)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| T-Mobile | 1900 - 1905 MHz | TDD | OCT 2004 – OCT 2024, not tradable |
| Tele 2 | 1905 - 1910 MHz | TDD | DEC 2004 – DEC 2024,not tradable |
| VIPnet | 1910 - 1915 MHz | TDD | OCT 2004 – OCT 2024,not tradable |

1. **Cyprus (March 2013)**

**1900-1920 MHz and 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequency band licensed** | **Technology in use (optional)** | **Licence duration, tradability** |
| CYTA | 1900-1905 MHz | UMTS | September 2005-February 2024, non-tradable |
| MTN | 1905-1910 MHz | UMTS | December 2004–December 2023, non-tradable |

1. **Czech Republic (March 2013)**

**1900-1920 MHz and 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequency band licensed** | **Technology in use (optional)** | **Licence duration, tradabilityx)** |
| T–Mobile Czech Republic, a.s. | 1910.1-1915.1 MHz | IMT/UMTS, TDD | 22. 10. 2024 |

1. **Denmark (March 2013)**

**1900-1920 MHz and 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequency band licensed** | **Technology in use (optional)** | **Licence duration, tradability** |
| TDC A/S | 1900-1905 MHz | TD SCDMA | Oct 2001 – Oct 2021, tradable |
| Telia Nättjanester Norden AB | 1905-1910 MHz | TD SCDMA | Oct 2001 – Oct 2021, tradable |
| Telenor A/S | 1910-1915 MHz | TD SCDMA | Dec 2005 – Oct 2021, tradable |
| HI3G Denmark ApS | 1915-1920 MHz | TD SCDMA | Oct 2001 – Oct 2021, tradable |

1. **Estonia (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| EMT AS | 1905.2-1910.0 MHz | TDD | 08.10.2012 (the validity of licence shall be extended once a year) Tradable |
| Elisa Eesti AS... | 1900.2-1905.0 MHz | TDD | 17.01.2013 (the validity of licence shall be extended once a year) Tradable |
| Tele2 Eesti AS | 1910.2-1915.0 MHz | TDD | 27.01.2013 (the validity of licence shall be extended once a year) Tradable |
| ProGroup Holding OÜ | 1915.2-1920.0 MHz | TDD | 30.01.2017  Tradable |

1. **Finland (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| TeliaSonera Finland Corp. | 1900.000 - 1904.800 MHz (Nationwide) | UTRA TFF | - 18.3.2019 |
| DNA Ltd. | 1905.000 - 1909.800 MHz  (Nationwide except Provence of Åland) | UTRA TDD | - 18.3.2019 |
| Elisa Corp. | 1910.000 - 1914.800 MHz  (Provence of Åland)  1915.000 - 1919.800 MHz  (Nationwide except Provence of Åland) | UTRA TDD | - 18.3.2019  - 18.3.2019 |
| Ålands Telekommunikation Ab | 1915.000 - 1919.800 MHz  (Provence of Åland) | UTRA TDD | - 18.3.2019 |

Note: in this table the term licence means a radio licence.

1. **France (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Bouygues Telecom | 1900.1-1905.1 MHz | UMTS – TDD  (not deployed) | 12 December 2002 – 11 December 2022, SRU tradable |
| Orange France | 1910.1-1915.1 MHz | UMTS – TDD  (not deployed) | 21 August 2001 – 20 August 2021,  SRU tradable |
| Société Française du radiotéléphone | 1915.1-1920.1 MHz | UMTS – TDD  (not deployed) | 21 August 2001 – 20 August 2021,  SRU tradable |

1. **Georgia (June, 2010)**

**1900-1920 MHz and 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequency band** | **Technology in use (optional)** | **Licence duration, tradability** |
| “Magticom” Ltd. | 1910.000-1915.000 MHz | UMTS-TDD | November 2006 – November 2016  tradable |
| “Magticom” Ltd. | 1915.000-1920.000 MHz | UMTS-TDD | September 2005 – September 2015,  tradable |
| “Geocell” Ltd. | 2010.000-2015.000 MHz | UMTS-TDD | June 2006 – June 2016  tradable |

1. **Germany (March 2013)**

**1900-1920 MHz and 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequency band licensed** | **Technology in use (optional)** | **Licence duration, tradability** |
| Telefónica Germany | 1900.1 – 1905.1 MHz |  | 31 December 2025 |
| E-Plus | 1905.1 – 1910.1 MHz |  | 31 December 2020 |
| Telekom Deutschland | 1910.1 – 1915.1 MHz |  | 31 December 2020 |
| Vodafone D2 | 1915.1 – 1920.1 MHz |  | 31 December 2020 |
| Telefónica Germany | 2010.5 – 2024.7 MHz |  | 31 December 2025 |

1. **Greece (January 2012)**

**1900-1920 MHz and 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequency band licensed** | **Technology in use (optional)** | **Licence duration,** |
| Cosmote | 1905.1 – 1910.1 MHz | UMTS | 05/08/2021 |
| Wind | 1910.1 – 1915.1 MHz | UMTS | 05/08/2021 |
| Vodafone | 1915.1 – 1920.1 MHz | UMTS | 05/08/2021 |

1. **Hungary (August 2012)**

**1900**-**1920 MHz / 2010**-**2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Telenor | 1905-1910 MHz | UTRA TDD | 31 12 2019  Extendable 7.5 years  Tradable with GSM1800 and UTRA FDD frequencies |
| Vodafone | 1910-1915 MHz | UTRA TDD | 31 12 2019  Extendable 7.5 years  Tradable with UTRA FDD frequencies |
| Magyar Telekom Nyrt. | 1915-1920 MHz | UTRA TDD | 31 12 2019  Extendable 7.5 years  Tradable with UTRA FDD frequencies |

1. **Iceland (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Nova ehf | 1900-1905 MHz | TDD | 30.3.2007-30.3.2022 |
| Síminn hf | 1915-1920 MHz | TDD | 30.3.2007-30.3.2022 |
| Og fjarskipti ehf | 1910-1915 MHz | TDD | 3.4.2007-3.4.2022 |

1. **Ireland (February 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Telefónica O2 Communications (Ireland) Limited | 1910-1915 MHx | UTRA TDD | October 2002 – October 2022  Not tradeable |

1. **Italy (March 2012)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequency band licensed** | **Technology in use (optional)** | **Licence duration, tradability** |
| H3G | 1900 – 1905 MHz | UMTS TDD | 31 december 2021 |
| VODAFONE | 1905 – 1910 MHz | UMTS TDD | 31 december 2021 |
| TELECOM ITALIA | 1910 – 1915 MHz | UMTS TDD | 31 december 2021 |
| WIND | 1915 – 1920 MHz | UMTS TDD | 31 december 2021 |

1. **Latvia (March 2013)**

**1900-1920 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Bite Latvija | 1900 – 1905 MHz | UMTS/IMT-2000/ TDD | June, 2020. Not tradable |
| Tele2 | 1905 – 1910 MHz | UMTS/IMT-2000/ TDD | December, 2017. Not tradable |
| Latvijas Mobilais Telefons (LMT) | 1915 – 1920 MHz | UMTS/IMT-2000/ TDD | December, 2017. Not tradable |

1. **Liechtenstein (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Orange (Liechtenstein) AG | 1905 - 1910 MHz | UMTS TDD | 31.12.2016  Not tradable |
| mobilkom liechtenstein AG | 1900 - 1905 MHz | UMTS TDD | Not limited  Not tradable |
| Swisscom (Schweiz) AG | 1915 - 1920 MHz | UMTS TDD | Not limited  Not tradable |

1. **Lithuania (January 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| **1900-1920 MHz / 2010-2025 MHz radio frequency bands are reserved. Permits are not issued.** | | | |

1. **Luxembourg (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | | | **Licence duration, tradability** |
| Entreprise des P&T | 1899.9-1904.9 MHz | | UMTS | 2017, not tradable | |
| Orange SA | 1904.9-1909.9 MHz | | UMTS | 2018, not tradable | |
| TANGO SA | 1909.9-1914.9 MHz | | UMTS | 2017, not tradable | |

1. **Former Yugoslav Republic of Macedonia (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| T-Mobile | 1910 – 1915 MHz | UTRA TDD | 17.12.2008 – 17.12.2018 tradable |

1. **Malta (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (paired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Vodafone Malta Ltd. | 1909.9-1914.9 MHz | UTRA TDD | Aug. 05 – Aug. 20,  not tradable |
| Mobisle Communications Ltd. | 1914.9-1919.9 MHz | UTRA TDD | Aug. 05 – Aug. 20,  not tradable |
| Melita Mobile Ltd. | 1904.9-1909.9 MHz | UTRA TDD | Aug. 07 – Aug. 22,  not tradable |

1. **Moldova (February 2011)**

**1900-1920 MHz and 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequency band licensed** | **Technology in use (optional)** | **Licence duration, tradability** |
| Orange Moldova | 1899.9-1904.9 MHz | UMTS TDD | August-2008 – August-2023,  non-tradable |
| Moldcell | 1914.9-1919.9 MHz | UMTS TDD | August-2008 – August-2023,  non-tradable |
| Moldtelecom | 1904.9-1909.9 MHz | UMTS TDD | December-2008 – December-2023,  non-tradable |

1. **Montenegro (March 2010)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Operator 1  (Promonte GSM) | 1905-1910 MHz | UTRA TDD | 13.04.2007. – 13.04.2022.  / tradable if approved by the NRA |
| Operator 2  (T-Mobile Crna Gora) | 1910-1915 MHz | UTRA TDD | 11.04.2007. – 11.04.2022.  / tradable if approved by the NRA |
| Operator 3  (MTEL) | 1915-1920 MHz | UTRA TDD | 21.04.2007. – 21.04.2022.  / tradable if approved by the NRA |

1. **The Netherlands (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| KPN | 1909.9 - 1914.9 MHz |  | Until Dec. 2016, tradable |
| T-mobile | 1900 – 1909.9 MHz  2010 – 2024.7 MHz |  | Until Dec. 2016, tradable |
| Vodafone | 1914.9 - 1920.3 MHz |  | Until Dec. 2016, tradable] |

1. **Norway (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Mobile Norway AS | 1900 – 1905 MHz | UMTS TDD | 01-01-2020, **tradable** |
| vacant | 1905 – 1920 MHz | Technology-neutral | n.a. |
| Inquam Norway AS | 2010 – 2025 MHz | Technology-neutral | 31-12-2022, **tradable** |

1. **Poland (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| POLKOMTEL S.A. | 1905.1-1910.1 MHz | UTRA TDD | 20.12.2000 – 01.01.2023 tradable |
| Polska Telefonia Cyfrowa Sp. z o.o. | 1910.1-1915.1 MHz | UTRA TDD | 20.12.2000 – 01.01.2023 tradable |
| Polska Telefonia Komórkowa ”Centertel” Sp. z o.o. | 1915.1-1920.1 MHz | UTRA TDD | 20.12.2000 – 01.01.2023 tradable] |
| P4 Sp. z o.o. | 1900.1-1905.1 MHz | UTRA TDD | Date 1 – 31.12.2023 tradable |

1. **Portugal (December 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability[[21]](#footnote-21)\*** |
| Not assigned | 1900 – 1920 MHz | ------------ | -------- |
|  |  |  |  |
| Not assigned | 2010 – 2025 MHz | --------- | -------- |

1. **Romania (June 2007)**

***IMT-2000/UMTS 2GHz Bands***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Operator** | **Licence start** | **Licence expiry (or duration)** | **Frequencies** | **Comments** |
| Vodafone Romania | March 2005 | March 2020 | FDD: 1964.9-1979.7 / 2154.9-2169.7 MHz  TDD: 1909.9-1914.9 MHz |  |
| Orange Romania | March 2005 | March 2020 | FDD: 1950.1-1964.9 / 2140.1-2154.9 MHz  TDD: 1904.9-1909.9 MHz |  |
| Telemobil | January 2007 | January 2022 | FDD: 1935.3-1950.1 / 2125.3-2140.1 MHz  TDD: 1899.9-1904.9 MHz |  |
| RCS&RDS | January 2007 | January 2022 | FDD: 1920.3-1935.3 / 2110.3-2125.3 MHz  TDD: 1914.9-1919.9 MHz |  |

1. **Russian Federation (September 2010)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| OJSC «Megafon» | 2010-2015 MHz | UTRA TDD | 2017 |
| OJSC «Mobile TeleSystems» | 2015-2020 MHz | UTRA TDD | 2017 |
| OJSC «VimpelCom» | 2020-2025 MHz | UTRA TDD | 2017 |

1. **Serbia (March 2010)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| TELEKOM SRBIJA | 1905 - 1910 MHz | UTRA TDD | 28.07.2006. – 28.07.2016., non-tradable |
| TELENOR | 1900 - 1905 MHz | UTRA TDD | 31.08.2006. – 31.08.2016., non-tradable |
| VIP MOBILE | 1910 - 1915 MHz | UTRA TDD | 10.11.2006. – 10.11.2016., non-tradable |

1. **Slovak Republic (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Orange Slovensko, a.s. | 1900 – 1905 MHz | TDD | 19.07.2002 – 31.08.2026, Tradable |
| Slovak Telekom, a.s | 1905 – 1910 MHz | TDD | 16.07.2002 – 31.08.2026, Tradable |
| Telefónica Slovakia, s.r.o. | 1910 - 1915 MHz | TDD | 07.09.2006 – 07.09.2026 , Tradable |

Note: This band is currently not in use.

1. **Slovenia (June 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| MOBITEL | 1900 – 1905 MHz | UMTS / TDD | 06.09.2004 – 27.11.2016 |
| T-2 | 1910 – 1915 MHz | UMTS / TDD | 21.09.2006 – 21.09.2021 |
| SI.MOBIL | 1915 – 1920 MHz | UMTS / TDD | 21.09.2006 – 21.09.2021 |

1. **Spain (March 2013)**

**1900-1920 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Orange | 1900.1-1905.1 MHz | UMTS TDD | Apr-’00 / apr-’20  tradable |
| Vodafone | 1905.1-1910.1 MHz | UMTS TDD | Apr-’00 / apr-’20  tradable |
| Telefónica | 1910.1 – 1915.1 MHz | UMTS TDD | Apr-’00 / apr-’20  tradable |
| Xfera (Yoigo) | 1915.1-1920.1 MHz | UMTS TDD | Apr-’00 / apr-’20  tradable |

1. **Sweden (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Svenska UMTS Licens AB (Tele2+TeliaSonera) | 1905.0 -1910.0 MHz | Not deployed | 16.12.2000 – 31.12.2025  tradable |
| HI3G Access AB | 1910.0 – 1915.0 MHz | Not deployed | 16.12.2000 – 31.12.2025  tradable |
| Telenor Sverige AB | 1915.0 – 1920.0 MHz | Not deployed | 16.12.2000 – 31.12.2025  tradable |

1. **Switzerland (July 2012)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Orange Networks SA | 1905.5 – 1910.5 MHz | [UTRA TDD] | JAN 01 – DEC 16  Not Tradable |
| Sunrise Communications AG | 1910.5 – 1915.5 MHz | [UTRA TDD] | JAN 01 – DEC 16  Not Tradable |
| Swisscom (Schweiz) AG | 1915.5 – 1920.5 MHz | [UTRA TDD] | JAN 01 – DEC 16  Not Tradable |
| Not assigned | 1900.5 – 1905.5 MHz  2010.0 – 2025.0 MHz |  |  |

1. **Turkey (January 2010)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| VODAFONE | 2010-2015 MHz | IMT/UMTS | 30 April 2009-30 April 2029  Not tradable |

1. **Ukraine (March 2010)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Ukrtelecom | 2015-2020 MHz | IMT-2000  CDMA  UMTS/WCDMA | Dec 2005 – Dec 2020 |

1. **United Kingdom (March 2013)**

**1900-1920 MHz / 2010-2025 MHz (unpaired frequency arrangement)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Operator** | **Frequencies** | **Technology in use (optional)** | **Licence duration, tradability** |
| Telefónica UK Ltd | 1909.9-1914.9 MHz | UTRA TDD | 1/4/2000 – 31/12/2021 Not tradable |
| Everything Everywhere Limited | 1899.9-1904.9 MHz | UTRA TDD | 1/4/2000 – 31/12/2021 Not tradable |
| Everything Everywhere Limited | 1904.9-1909.9 MHz | UTRA TDD | 1/4/2000 – 31/12/2021 Not tradable |
| Hutchison 3G UK Ltd. | 1914.9 - 1920.0 MHz | UTRA TDD | 1/4/2000 – 31/12/2021 Not tradable |

1. Typical Technical Characteristics for ENG/OB Links (Extracted from ERC Recommendation 25-10)

Table 5: Recommended frequency ranges for use by audio and video SAP/SAB links

| **Type of link** | **Recommended frequencies** | | **Technical parameters** |
| --- | --- | --- | --- |
| **Tuning ranges** | **Preferred sub-bands** |
| Radio microphones and  In-ear monitors | 174-216 MHz  470-862 MHz  1785-1800 MHz  (Note 1) | 1785-1800 MHz | ERC/REC 70-03 |
| Portable audio links and  Mobile audio links and  Temporary point-to-point audio links | VHF/UHF (Note 2) | None | ERC Report 42 |
| Cordless cameras | 2025-2110/2200-2500 MHz  10.0-10.60 GHz  21.2-24.5 GHz  47.2-50.2 GHz | 10.3-10.45 GHz  21.2-21.4 GHz, 22.6-23.0 GHz and 24.25-24.5 GHz | ERC Report 38 |
| Portable video links | 2025-2110/2200-2500 MHz  2500-2690 MHz (Note 4)  10.0-10.60 GHz | 10.3-10.45 GHz | ERC Report 38 |
| Mobile video links  (airborne and vehicular) | 2025-2110/2200-2500 MHz  2500-2690 MHz (Note 4)  3400-3600 MHz (Note 5) |  | ERC Report 38 |
| Temporary point-to-point video links | Fixed service bands (Note 6)  10.0-10.68 GHz (Note 3)  21.2-24.5 GHz | 10.3-10.45 GHz  21.2-21.4 GHz, 22.6-23.0 GHz and 24.25-24.5 GHz | ERC Report 38 |

**Note 1:** The band 863-865 MHz is available for radio microphones, however due note should be taken that it is used also for non-professional and consumer radio applications (cordless audio, etc.).

**Note 2:** Depending on application scenario, channel width and required transmitter power, the portable, mobile and temporary point-to-point audio links may be accommodated either in the frequency bands 174-216 MHz/470-862 MHz identified for professional radio microphones (typically for low power/wideband applications) or in other VHF/UHF bands, including Private Mobile Radio (PMR) bands (typically for high power/narrowband applications).

**Note 3:** Only occasional temporary point-to-point links should be allowed in the frequency band 10.6-10.68 GHz. Studies have concluded that even limited deployment of cordless cameras and portable video links in the band 10.6-10.68 GHz will result in interference to the EESS (passive) services using this band (see ECC Report 017 [24]).

**Note 4:** The band 2500-2690 MHz will not be available for video SAP/SAB links after the introduction of UMTS/IMT-2000 (see ECC/DEC/(02)06 [25] ).

**Note 5:** In countries where the band 3400-3600 MHz is widely used for Fixed Wireless Access (FWA), availability of this band for mobile video SAP/SAB links may be restricted.

**Note 6:** Temporary point-to-point video links are often accommodated in the traditional fixed services’ bands, following the same channel arrangements as the FS links.

1. Typical Technical Characteristics for ENG/OB Links (Extracted from ERC Report 38

Table 6: Typical Technical Characteristics for ENG/OB Links

| **Type of Link** | **Range** | **Max e.i.r.p.** | **Min  Tx ant. gain** | **Min**  **Rx ant. gain** | **Radio Link Path** | **Suitable Frequency Range** | **Description** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Cordless Camera** | <500m | 6dBW  13dBW  (22 GHz or 47GHz) | 0dBi | 6dBi | Usually clear line of sight. | Currently < 12 GHz but future systems at 22GHz and 47GHz may be achievable. | Handheld camera with integrated transmitter, power pack and antenna. |
| **Portable link** | <2km | 16dBW | 6dBi | 17dBi | Not always clear line of sight. | <5GHz | Handheld camera but with separate bodyworn transmitter, power pack and antenna. |
| **Mobile link** | <10km | 26dBW | 3dBi | 13dBi | Often obstructed and susceptible to multipath impairment. | <5GHz | Mounted in helicop­ters, motorcycles, pedal cycles, cars, racing cars and boats. One or both link terminals may be used when moving. |
| **Temporary point-to-point**  **link** | <80km  each hop  for links at  <10GHz | 40dBW | 13dBi | 17dBi | Usually clear line of sight for OB, but often obstructed for ENG use. | <10GHz for long hops.  Hop length at >10GHz limited by precipitation fading. | Link terminals are mounted on tripods, temporary platforms, purpose built vehicles or hydraulic hoists.  Two-way links are often required. |

1. List of references
2. CEPT Report 014 Report from CEPT to the European Commission in response to the Mandate to: Develop a strategy to improve the effectiveness and flexibility of spectrum availability for Short Range Devices (SRDs)
3. CEPT Report 044 In response to the EC Permanent Mandate on the ”Annual update of the technical annex of the Commission Decision on the technical harmonisation of radio spectrum for use by short range devices”
4. ERC Decision (99)25 on the harmonised utilisation of spectrum for terrestrial Universal Mobile Telecommunications System (UMTS) operating within the bands 1900 - 1980 MHz, 2010 - 2025 MHz and 2110 - 2170 MHz
5. ERC Decision (00)01 on the frequency bands for the introduction of terrestrial Unversal Mobile Telecommunications System (UMTS)
6. ERC Decision (97)07 on the frequency bands for the introduction of the Universal Mobile Telecommunications System (UMTS)
7. ECC Decision (06)01 on the harmonised utilisation of spectrum for terrestrial IMT-2000/UMTS systems operating within the bands1900-1980 MHz, 2010-2025 MHz and 2110-2170 MHz
8. ECC Decision (13)01 on the use, free circulation, and exemption from individual licensing of Earth stations on mobile platforms (ESOMPs) in the frequency bands available for use by uncoordinated FSS Earth stations within the ranges 17.3-20.2 GHz and 27.5-30.0 GHz
9. Decision 128/1999/EC of the European Parliament and the Council, dated 14 December 1998, on the coordinated introduction of a third-generation mobile and wireless communications system (UMTS) in the Community
10. ECO Report 03: The licensing of 'Mobile bands' in CEPT
11. CEPT Report 019 Report from CEPT to the European Commission in response to   
    EC Mandate to develop least restrictive technical conditions for frequency bands addressed in the context of WAPECS
12. CEPT Report 039 Report from CEPT to the European Commission in response to the Mandate to develop least restrictive technical conditions for 2 GHz bands
13. ERC Report 64 Sharing between UMTS and existing fixed services
14. ERC Report 65 Adjacent band compatibility between UMTS and other 2 GHz services
15. ERC Report 25 European Common Allocation Table
16. ETSI EN 301 908-10 Electromagnetic compatibility and Radio spectrum Matters (ERM);Base Stations (BS), Repeaters and User Equipment (UE) for IMT-2000 Third-Generation cellular networks;Part 10: Harmonised EN for IMT-2000, FDMA/TDMA (DECT) covering essential requirements of article 3.2 of the R&TTE Directive
17. ETSI EN 300 175 (several parts): Digital Enhanced Cordless Telecommunications (DECT);Common Interface (CI)
18. ERC Recommendation 25-10 on frequency ranges for the use of temporary terrestrial audio and video SAP/SAB links (incl. ENG/OB)
19. ECC Report 002 SAP/SAB (Incl. ENG/OB) spectrum use and future requirements
20. ERC Report 38 Handbook on radio equipment and systems video links for ENG/OB use
21. ERC Recommendation T/R 22-02
22. Decision ERC/DEC/(94)03 on the frequency band to be designated for the coordinated introduction of the Digital European Cordless Telecommunications system
23. Decision ERC/DEC/(98)22 on Exemption from Individual Licensing of DECT equipment, except fixed parts which provide for public access (Corrected 30 March 2007); this decision is currently under revision in CEPT
24. ECC Report 199 user requirements and spectrum needs for the future European broadband PPDR system (Wide Area Network)
25. ECC Report 017 Sharing between EESS (Passive) and video SAP/SAB links in the band 10.6-10.68 GHz
26. ECC/DEC/(02)06 on the designation of frequency band 2500-2690 MHz for UMTS/IMT-2000
27. FM48(13)045 - Annex 4 Draft ECC Report on Broadband Direct-Air-to-Ground Communications (DA2GC)
28. ECC Report 209: Compatibility/sharing studies related to Broadband Direct-Air-to-Ground Communications (DA2GC) in the frequency bands 1900 – 1920 MHz / 2010 – 2025 MHz and services/applications in the adjacent bands
29. ECC Report 210 on Compatibility/sharing studies related to Broadband Direct-Air-to-Ground Communications (DA2GC) in the frequency bands 5855-5875 MHz, 2400-2483.5 MHz and 3400 – 3600 MHz
30. Draft ECC Report on Compatibility between DA2GC and PMSE video links in the 2 GHz unpaired bands
31. ECC Report 189: Future Spectrum Demand for Short Range Devices in the UHF Frequency Bands
32. ETSI TR 103 054 V1.1.1 (2010-07), System Reference Document on Broadband Direct-Air-to-Ground Communications operating in part of the frequency range from 790 MHz to 5150 MHz; FM48(10)003
33. ETSI TR 101 599 V1.1.3 (2012-09), System Reference Document on Broadband Direct-Air-to-Ground Communications System employing beamforming antennas, operating in the 2.4 GHz and 5.8 GHz bands; FM48(12)036
34. ETSI TR 103 108 V1.1.1 (2013-07), System Reference Document on Broadband Direct-Air-to-Ground Communications System operating in the 5.855 GHz to 5.875 GHz band using 3G technology
35. ETSI TR 103 149 V1.1.1 (2013-09): System Reference Document on DECT operating in the 1 900 MHz - 1 920 MHz band
36. FM(14)021\_ECO Summary of Consultation of the Call for Inputs for the 2 GHz Unpaired Bands

1. http://www.eurocontrol.int/articles/statistics-and-forecasts. [↑](#footnote-ref-1)
2. http://imsresearch.com/news-events/press-template.php?pr\_id=1981. [↑](#footnote-ref-2)
3. Programme Making includes the making of a programme for broadcast, the making of a film, presentation, advertisement or audio or video recordings, and the staging or performance of an entertainment, sporting or other public event. [↑](#footnote-ref-3)
4. A Special Event is an occurrence of limited duration, typically between one day and a few weeks, which take place on specifically defined locations. Examples include large cultural, sport, entertainment, religious and other festivals, conferences and trade fairs. In the entertainment industry, theatrical productions may run for considerably longer. [↑](#footnote-ref-4)
5. For further information see the ECC Report 002 [18] [↑](#footnote-ref-5)
6. Council Directive on the frequency band to be designated for the coordinated introduction of digital European cordless telecommunications (DECT) into the Community (91/287/EEC) (Annex 1 to ERC/DEC/(94)03) [21]. [↑](#footnote-ref-6)
7. Decision 128/1999/EC of the European Parliament and of the Council of 14 December 1998 on the coordinated introduction of a third-generation mobile and wireless communications system (UMTS) in the Community [↑](#footnote-ref-7)
8. Mandate to CEPT on the 2 GHz bands: <http://ec.europa.eu/information_society/policy/ecomm/radio_spectrum/_document_storage/mandates/2009mandate_2ghz.pdf> [↑](#footnote-ref-8)
9. Document RSCOM10-25 [↑](#footnote-ref-9)
10. Decision 676/2002/EC of the European Parliament and of the Council of 7 March 2002 on a regulatory framework for radio spectrum policy in the European Community, OJL 108 of 24.4.2002 [↑](#footnote-ref-10)
11. Only the licence conditions of operators in Austria (upon request), Germany, the Netherlands, and Sweden allow technology neutral use of the terrestrial 2 GHz band or parts thereof (see RSCOM12-05) [↑](#footnote-ref-11)
12. As recognised in CEPT Report 39 [↑](#footnote-ref-12)
13. Article 8 of the RSPP [↑](#footnote-ref-13)
14. In this regard, the Commission issued on 15 December 2011 a mandate to CEPT (RSCOM11-59) to identify suitable frequency bands for PMSE (still ongoing). [↑](#footnote-ref-14)
15. See <http://ec.europa.eu/information_society/policy/ecomm/radio_spectrum/get_involved/activities/index_en.htm#ongoing_consultations> [↑](#footnote-ref-15)
16. The order in this shortlist is chosen arbitrarily. [↑](#footnote-ref-16)
17. Including innovative applications such as M2M [↑](#footnote-ref-17)
18. Reported in documents FM(12)084 Annex 58 and ECC PT1(12)048 [↑](#footnote-ref-18)
19. DECT is considered to be an application with the potential to address the priority given to the Internet of Things set out in Article 8 of the RSPP. [↑](#footnote-ref-19)
20. Subject to subsequent public consultation [↑](#footnote-ref-20)
21. \* The rights of use of spectrum set out in the NTFA (National Table of Frequency Allocations) are transferable in accordance with the Law of Electronic Communications (<http://www.anacom.pt/render.jsp?categoryId=97279#horizontalMenuArea>) - See article nº 34 of [Law no. 51/2011, of 13 September](http://www.anacom.pt/render.jsp?contentId=1099877) [↑](#footnote-ref-21)