**CODING PROTOCOL:**

The coding protocol for PLB equipment licensed in Cyprus is SERIAL USER PROTOCOL. The number is assigned by the competent authority (JRCC Larnaca) upon request prior the registration. Certification of programming must be presented for registration to be valid